{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","","","30","34"]
["","","Ogrzewanie","Bardzo niska","m³/min","","","32","34"]
["Poziom mocy akustycznej","Ogrzewanie","","","dBA","","62","","","62"]
["","Chłodzenie","","","dBA","","60","","","60"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","cfm","","","1059","1200"]
["","","Ogrzewanie","Bardzo niska","cfm","","","1130","1200"]
["Wymiary","Jednostka","","Wysokość","mm","550","550","550","550","550","550"]
["","","","Szerokość","mm","765","765","765","765","765","765"]
["","","","Głębokość","mm","285","285","285","285","285","285"]
["Ciężar","Jednostka","","","kg","36","36","36","41","41","41"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min","500","500","760","890","500","500"]
["","","Ogrzewanie","Bardzo niska","obr/min","320","320","820","890","500","500"]
["Compressor","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","46.0","-10","-10","46.0"]
["","","","Maks.","°CDB","","-10","46","46","-10"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","-15","-15","-15","-15.0"]
["","","","Maks.","°CWB","","18.0","18","18","18.0"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","46","46","","","48","48"]
["","","","Nom.","dBA","","","48","46"]
["","Grzanie","","Wysoki","dBA","48","48","","","50","50"]
["","","","Nom.","dBA","","","50","48"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Ilość","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Ilość","","","tCO2Eq","0.59","0.6","0.6","0.8","0.78","0.78"]
["","GWP","","","","675.0","675","675","675","675","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20 (1)","20","20","20 (1)","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","002 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15.0","15","15","15","15","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","30","30","30","30","30","30"]
["Standardowe akcesoria","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50","50"]
["","Napięcie","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Uwagi","","","","","(1) - Dla jednego pomieszczenia","","(1) - Zawiera fluorowane gazy cieplarniane","","","(1) - Dla jednego pomieszczenia"]
["","","","","","","(1) - Dla jednego pomieszczenia","","","(1) - Dla jednego pomieszczenia"]
["","","","","","","(2) - Patrz oddzielny rysunek zakresu pracy","","","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","","","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","","(4) - Zawiera fluorowane gazy cieplarniane","","","(4) - Zawiera fluorowane gazy cieplarniane"]
["Sprężarka","Typ","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Standardowe akcesoria","Reducer assembly","","","","","","","1","1","1"]