{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M9"]
[]
[]
[]
[]
["","","","","","2AMXM40M4V1B9","2AMXM50M4V1B9"]
["Wymiary","Jednostka","","Wysokość","mm","552","552"]
["","","","Szerokość","mm","852","852"]
["","","","Głębokość","mm","350","350"]
["Ciężar","Jednostka","","","kg","36","41"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","500","500"]
["","","Ogrzewanie","Bardzo niska","obr/min_","320","500"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","46","48"]
["","Grzanie","","Wysoki","dBA","48","50"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32"]
["","Ilość","","","kg","0.88","1.15"]
["","Ilość","","","tCO2Eq","0.60","0.78"]
["","GWP","","","","675","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20 (1)","20 (1)"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","30","30"]
["Standardowe akcesoria","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-230-240","220-230-240"]
["Uwagi","","","","","(1) - Dla jednego pomieszczenia","(1) - Dla jednego pomieszczenia"]
["Standardowe akcesoria","Reducer assembly","","","","","1"]