{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","30","","","34"]
["","","Ogrzewanie","Bardzo niska","m³/min","32","","","34"]
["","","","Bardzo niska","cfm","1059","","","1200"]
["","","Ogrzewanie","Bardzo niska","cfm","1130","","","1200"]
["Wymiary","Jednostka","","Wysokość","mm","550","550","550","550"]
["","","","Szerokość","mm","765","765","765","765"]
["","","","Głębokość","mm","285","285","285","285"]
["Ciężar","Jednostka","","","kg","36","36","36","41"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min","760","500","500","890"]
["","","Ogrzewanie","Bardzo niska","obr/min","820","320","320","890"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10","-10 (2)","-10"]
["","","","Maks.","°CDB","46","46","46 (2)","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","46","46"]
["","","","Nom.","dBA","48","","","46"]
["","Grzanie","","Wysoki","dBA","","48","48"]
["","","","Nom.","dBA","50","","","48"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32"]
["","Ilość","","","kg","0.88","0.88","0.88","1.15"]
["","Ilość","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["","GWP","","","","675","675","675","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20","20 (1)","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15","15.0","15.0","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","30","30","30","30"]
["Standardowe akcesoria","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","220-240","220-230-240","220-230-240","220-240"]
["Uwagi","","","","","","(1) - Dla jednego pomieszczenia"]
["","","","","","","","(1) - Dla jednego pomieszczenia"]
["","","","","","","","(2) - Patrz oddzielny rysunek zakresu pracy"]
["Standardowe akcesoria","Reducer assembly","","","","","","","1"]