{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Poziom ciśn. akust.","Grzanie","","Nom.","dBA","48","48","","50","50"]
["","Chłodzenie","","Nom.","dBA","47","47","","48","48"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1","","1","1"]
["","Torebka ze śrubami","","","","1","1","","1","1"]
["","Korek spustowy","","","","1","1","","1","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","kg","1.20","1.20","","1.60","1.60"]
["","Typ","","","","R-410A","R-410A","","R-410A","R-410A"]
["Połączenia instalacji rurowej","Różnica poziomów","IU - IU","Maks.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15","","15","15"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","0,02 (dla długości instalacji rurowej przekraczającej 20 m)"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","30","30","","30","30"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","765","765","","765","765"]
["","","","Głębokość","mm","285","285","","285","285"]
["","","","Wysokość","mm","550","550","","550","550"]
["Ciężar","Jednostka","","","kg","38","38","","42","42"]
["Power supply","liczba faz","","","","1~","1~","","1~","1~"]
["","Częstotliwość","","","Hz","50","50","","50","50"]
["","Napięcie","","","V","220-240","220-240","","220-240","220-240"]
["Uwagi","","","","","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane","","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane"]
["Wymiary","Jednostka","","Wysokość","mm","","","550","","","550"]
["","","","Szerokość","mm","","","765","","","765"]
["","","","Głębokość","mm","","","285","","","285"]
["Ciężar","Jednostka","","","kg","","","38","","","42"]
["Sprężarka","Typ","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","","10","","","10"]
["","","","Maks.","°CDB","","","46","","","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","","-15","","","-15"]
["","","","Maks.","°CWB","","","15.5","","","15.5"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","","","47","","","48"]
["","Grzanie","","Nom.","dBA","","","48","","","50"]
["Czynnik chłodniczy","Typ","","","","","","R-410A","","","R-410A"]
["","Ilość","","","kg","","","1.20","","","1.60"]
["","Ilość","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","","20","","","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","","0,02 (dla długości instalacji rurowej przekraczającej 20 m)","","","0,02 (dla długości instalacji rurowej przekraczającej 20 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","","","15","","","15"]
["","","IU - IU","Maks.","m","","","7.5","","","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","","","30","","","30"]
["Standardowe akcesoria","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","","","1~","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","50","","","50"]
["","Napięcie","","","V","","","220-240","","","220-240"]
["Standardowe akcesoria","Zespół reduktora","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]