{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","47"]
["","Chłodzenie","","Nom.","dBA","46"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1"]
["","Torebka ze śrubami","","","","1"]
["","Korek spustowy","","","","1"]
["","Nasadka spustowa (1)","","","","6"]
["","Nasadka spustowa (2)","","","","3"]
["","Odlepiana etykieta o gazach fluorowanych","","","","1"]
["","Dodatkowa klasa chłodzenia","","","","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Ilość","","","kg","1.8"]
["","Typ","","","","R-32"]
["Fan motor","Prędkość","Chłodzenie","Bardzo niska","obr/min_","420"]
["","","Grzanie","Bardzo niska","obr/min_","420"]
["Połączenia instalacji rurowej","Różnica poziomów","IU - IU","Maks.","m","7.5"]
["","","IU - OU","Maks.","m","15"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","50"]
["Sprężarka","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","868"]
["","","","Głębokość","mm","320"]
["","","","Wysokość","mm","734"]
["Ciężar","Jednostka","","","kg","57"]
["Power supply","liczba faz","","","","1~"]
["","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]
["Uwagi","","","","","(1) - Zawiera fluorowane gazy cieplarniane"]
["","","","","","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","","24"]
["","","Ogrzewanie","Bardzo niska","m³/min","","24"]
["","","","Bardzo niska","cfm","","847"]
["","","Ogrzewanie","Bardzo niska","cfm","","847"]
["Wymiary","Jednostka","","Wysokość","mm","","734"]
["","","","Szerokość","mm","","868"]
["","","","Głębokość","mm","","320"]
["Ciężar","Jednostka","","","kg","","57"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","","420"]
["","","Ogrzewanie","Bardzo niska","obr/min_","","420"]
["Sprężarka","Type","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","-10"]
["","","","Maks.","°CDB","","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","-15"]
["","","","Maks.","°CWB","","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","","46"]
["","Grzanie","","Nom.","dBA","","47"]
["Czynnik chłodniczy","Typ","","","","","R-32"]
["","Ilość","","","kg","","1.80"]
["","Ilość","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","25"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","","15"]
["","","IU - IU","Maks.","m","","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","","50"]
["Standardowe akcesoria","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","220-240"]