{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXF-A9"]
[]
[]
[]
[]
["","","","","","3MXF52A2V1B9","3MXF68A2V1B9"]
["Wymiary","Jednostka","","Wysokość","mm","734","734"]
["","","","Szerokość","mm","974","974"]
["","","","Głębokość","mm","401","401"]
["Ciężar","Jednostka","","","kg","57","62"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","420","420"]
["","","Ogrzewanie","Bardzo niska","obr/min_","420","300"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","46","48"]
["","Grzanie","","Nom.","dBA","47.0","48.0"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32"]
["","Ilość","","","kg","1.8","2"]
["","Ilość","","","tCO2Eq","1.22","1.35"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","25 (1)","25 (1)"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","002 (dla długości instalacji rurowej przekraczającej 30 m)","002 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","50","50"]
["Standardowe akcesoria","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Zakres efektywności energetycznej","","","","","A+++ ~ D","A+++ ~ D"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - Dla jednego pomieszczenia","(1) - Dla jednego pomieszczenia"]
["","","","","","(2) - Patrz oddzielny rysunek zakresu pracy","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","(4) - Zawiera fluorowane gazy cieplarniane","(4) - Zawiera fluorowane gazy cieplarniane"]