{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N8"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B8","3MXM52N2V1B8"]
["Wymiary","Jednostka","","Wysokość","mm","734","734"]
["","","","Szerokość","mm","974","974"]
["","","","Głębokość","mm","401","401"]
["Ciężar","Jednostka","","","kg","57","57"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr./min","420","420"]
["","","Ogrzewanie","Bardzo niska","obr./min","420","420"]
["Compressor","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","46","46"]
["","Grzanie","","Nom.","dBA","47.0","47.0"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32"]
["","Ilość","","","kg","1.8","1.8"]
["","Ilość","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675.0","675.0"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","25","25"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 30 m)","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","50","50"]
["Standardowe akcesoria","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - Dla jednego pomieszczenia","(1) - Dla jednego pomieszczenia"]
["","","","","","(2) - Możliwość połączenia z CVXM-A, FVXM-A - maksymalna długość instalacji rurowej wynosi 30 m.","(2) - Możliwość połączenia z CVXM-A, FVXM-A - maksymalna długość instalacji rurowej wynosi 30 m."]