{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-K"]
[]
[]
[]
[]
["","","","","","3MXS40K3V1B","3MXS40K3V1B2","3MXS40K2V1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","47","47"]
["","Chłodzenie","","Nom.","dBA","46","46"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1"]
["","Korek spustowy","","","","1","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Dopełnienie","","","kg","2.0","2.0"]
["","Typ","","","","R-410A","R-410A"]
["Połączenia instalacji rurowej","Różnica poziomów","IU - IU","Maks.","m","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 30 m)","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","50","50"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","936","936"]
["","","","Głębokość","mm","300","300"]
["","","","Wysokość","mm","735","735"]
["Ciężar","Jednostka","","","kg","49","49"]
["Power supply","Phase","","","","1~","1~"]
["","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","230","230"]
["Uwagi","","","","","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane"]
["Wymiary","Jednostka","","Wysokość","mm","","","735"]
["","","","Szerokość","mm","","","936"]
["","","","Głębokość","mm","","","300"]
["Ciężar","Jednostka","","","kg","","","49"]
["Sprężarka","Typ","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","","-15"]
["","","","Maks.","°CWB","","","15.5"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","","","46"]
["","Grzanie","","Nom.","dBA","","","47"]
["Czynnik chłodniczy","Typ","","","","","","R-410A"]
["","Ilość","","","kg","","","2.0"]
["","Ilość","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","","50"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","","","15"]
["","","IU - IU","Maks.","m","","","7.5"]
["Standardowe akcesoria","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","50"]
["","Napięcie","","","V","","","230"]