{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B","4MXS80E3V3B2","4MXS80E7V3B"]
["Wymiary","Jednostka","","Wysokość","mm","770","770"]
["","","","Szerokość","mm","900","900"]
["","","","Głębokość","mm","320","320"]
["Ciężar","Jednostka","","","kg","72","72"]
["Sprężarka","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Poziom ciśn. akust.","Chłodzenie","","Nom.","dBA","48","48"]
["","Grzanie","","Nom.","dBA","49","49"]
["Czynnik chłodniczy","Typ","","","","R-410A","R-410A"]
["","Ilość","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Połączenia instalacji","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 30 m)","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","70","70"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1"]
["","Korek spustowy","","","","1","1"]
["","Zespół reduktora","","","","1","1"]
["Power supply","Phase","","","","1~","1~"]
["","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","230","230"]
["Uwagi","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB; długość równoważna instalacji rurowej: 7,5 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB; długość równoważna instalacji rurowej: 7,5 m"]
["","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m"]
["","","","","","(3) - Zawiera fluorowane gazy cieplarniane","(3) - Zawiera fluorowane gazy cieplarniane"]
["Wymiary","Jednostka","","Wysokość","mm","","","770"]
["","","","Szerokość","mm","","","900"]
["","","","Głębokość","mm","","","320"]
["Ciężar","Jednostka","","","kg","","","72"]
["Sprężarka","Type","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","","-15"]
["","","","Maks.","°CWB","","","15.5"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","","","48"]
["","Grzanie","","Nom.","dBA","","","49"]
["Czynnik chłodniczy","Typ","","","","","","R-410A"]
["","Ilość","","","kg","","","2.99"]
["","Ilość","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","","25"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","","","15"]
["","","IU - IU","Maks.","m","","","7.5"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","","","70"]
["Standardowe akcesoria","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","50"]
["","Napięcie","","","V","","","230"]