{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Wymiary","Jednostka","","Wysokość","mm","734","734"]
["","","","Szerokość","mm","1,040","1,040"]
["","","","Głębokość","mm","408","408"]
["Ciężar","Jednostka","","","kg","69","73"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","48","52"]
["","Grzanie","","Nom.","dBA","49","53"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32"]
["","Ilość","","","kg","2","2.4"]
["","Ilość","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","25 (2)","25 (3)"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 30 m)","0,02 (dla długości instalacji rurowej przekraczającej 30 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15 (3)","15"]
["","","IU - IU","Maks.","m","7.5 (3)","7.5 (3)"]
["","Całkowita długość instalacji","System","Rzeczywisty","m","60","75"]
["Standardowe akcesoria","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-440","220-240"]
["Uwagi","","","","","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(2) - Dla jednego pomieszczenia","(2) - Dla jednego pomieszczenia"]
["","","","","","(3) - Dla jednego pomieszczenia (w przypadku kombinacji z FBA71/100/125 oraz EKHWET i CKHWS patrz instrukcja instalacji)","(3) - Dla jednego pomieszczenia (w przypadku kombinacji z FBA71/100/125 oraz EKHWET i CKHWS patrz instrukcja instalacji)"]
["","","","","","(4) - Zawiera fluorowane gazy cieplarniane","(4) - Zawiera fluorowane gazy cieplarniane"]