{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Wydajność chłodnicza","Nom.","","kW","9.5","12.1 (1)"]
["Chłodzenie pomieszczeń","SEER","","","4.65","4.68"]
["","Roczne zużycie energii","","kWh/rok","716","1,550"]
["","Wydajność","Pdesign","kW","9.50","12.1"]
["","Klasa efektywności energetycznej","","","B"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Wydajność","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Klasa efektywności energetycznej","","","A"]
["","Roczne zużycie energii","","kWh/rok","2,498","3,340"]
["Efektywność nominalna","Rocz. zużycie ener.","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","D"]
["","","Ogrzewanie","","B"]
["Wydajność grzewcza","Nom.","","kW","10.8","13.5 (2)"]
["Uwagi","","","","(1) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewn. 35°CDB; długość równoważna instalacji rurowej: 7,5m; różnica poziomów: 0 m"]
["","","","","(2) - Roczne zużycie energii jest zgodne z Dyrektywą na temat oznaczeń konsumpcji energii 2002/31/WE","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 7,5 m; różnica poziomów: 0 m"]
["","","","","(3) - Współczynniki SEER i SCOP zgodne z EN 14825","(3) - Wartości EER/COP według Eurovent 2012, do użytkowania tylko poza Unią Europejską"]
["","","","","(4) - Wydaj. znam.: (chłodzenie przy temp. 35°/27° i obciążeniu znam., grzanie przy temp. 7°/20° i obciążeniu znam.)"]