{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standardowe akcesoria","Instrukcja instalacji","","","","Instrukcja instalacji"]
["","Instrukcja obsługi","","","","Instrukcja obsługi"]
["","Śruba +podkładka","","","","Śruba +podkładka"]
["","Pilot bezprzewodowy","","","","Pilot bezprzewodowy"]
["","Kratka blokady pokrywy","","","","Kratka blokady pokrywy"]
["","Bateria","","","","Bateria"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52"]
["","Gaz","","Śr. zewn.","mm","15.88"]
["","Spust","","","","19.05"]
["Power input","Chłodzenie","","Nom.","kW","0.128"]
["","Grzanie","","Nom.","kW","0.128"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","64"]
["","Ogrzewanie","","","dBA","64"]
["Wymiary","Jednostka","","Szerokość","mm","600"]
["","","","Głębokość","mm","1,007"]
["","","","Wysokość","mm","285"]
["Obudowa","Materiał","","","","Stal galwanizowana"]
["Ciężar","Jednostka","","","kg","35"]
["Wentylator","Ciśnienie statyczne zewnętrzne","","Wysokie","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Niskie","Pa","64"]
["Power supply","liczba faz","","","","1~"]
["","Częstotliwość","","","Hz","50"]
["","Nazwa","","","","V1"]
["","Napięcie","","","V","220-240"]
["Pobór mocy","Grzanie","","Nom.","kW","","0.109"]
["","Chłodzenie","","Nom.","kW","","0.109"]
["Wentylator","Spręż dyspozycyjny","","Wysokie","Pa","","70","150","150"]
["","","","Niskie","Pa","","45","111","92"]
["Obudowa","Materiał","","","","","Stal galwanizowana"]
["Wymiary","Jednostka","","Wysokość","mm","","378","378","378"]
["","","","Szerokość","mm","","541","1300","1500"]
["","","","Głębokość","mm","","1045","541","541"]
["Ciężar","Jednostka","","","kg","","44","50","56"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Niski","m³/min","","18.3","34.8","37.9"]
["","","Grzanie","Wysoki","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Niski","m³/min","","18.3","34.8","37.9"]
["","Spręż dyspozycyjny","","Nom.","Pa","","57","128","122"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","60","72","73"]
["","Ogrzewanie","","","dBA","","60","72","73"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Niski","dBA","","36","50","50"]
["","Grzanie","","Wysoki","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Niski","dBA","","36","50","50"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","","15.88","15.9","15.9"]
["","Spust","","","","","19.05"]
["Standardowe akcesoria","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Zasilanie energią elektryczną","liczba faz","","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","220-240"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","","","12.10","13.00"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","","","13.5","15.5"]
["Obudowa","Kolor","","","","","","Stal galwanizowana / niemalowana","Stal galwanizowana / niemalowana"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","","37","44"]
["","","Ogrzewanie","Czynnik","m³/min","","","37.4","43.9"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Czynnik","dBA","","","52","53"]
["","Ogrzewanie","","Czynnik","dBA","","","52","53"]
["Syst. kontroli","Pilot na podczerwień","","","","","","ARCWLA","ARCWLA"]