{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Cicha praca","dBA","","36","","41"]
["","","","Niski","dBA","","38","","43"]
["","Chłodzenie","","Cicha praca","dBA","","36","","41"]
["","","","Niski","dBA","","38","","43"]
["","","","Wysoki","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standardowe akcesoria","Instrukcja instalacji","","","","","Instrukcja instalacji","","Instrukcja instalacji"]
["","Instrukcja obsługi","","","","","Instrukcja obsługi","","Instrukcja obsługi"]
["","Śruby","","","","","Śruby","","Śruby"]
["","Podkładka","","","","","Podkładka","","Podkładka"]
["","Pilot bezprzewodowy","","","","","Pilot bezprzewodowy","","Pilot bezprzewodowy"]
["","Kratka blokady pokrywy","","","","","Kratka blokady pokrywy","","Kratka blokady pokrywy"]
["","Bateria","","","","","Bateria","","Bateria"]
["Syst. kontroli","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Ciecz","","Śr. zewn.","mm","","9.52","","9.52"]
["","Gaz","","Śr. zewn.","mm","","15.88","","15.88"]
["","Spust","","","","","19.05","","19.05"]
["Power input","Chłodzenie","","Nom.","kW","","0.094","","0.137"]
["","Grzanie","","Nom.","kW","","0.094","","0.137"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","56","","60"]
["","Ogrzewanie","","","dBA","","56","","60"]
["Wymiary","Jednostka","","Szerokość","mm","","820","","820"]
["","","","Głębokość","mm","","820","","820"]
["","","","Wysokość","mm","","300","","300"]
["Obudowa","Materiał","","","","","Stal galwanizowana","","Stal galwanizowana"]
["Ciężar","Jednostka","","","kg","","39","","39"]
["Wentylator","Przepływ powietrza","Grzanie","Wysoki","m³/min","","29.2","","34.0"]
["","","","Niski","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Chłodzenie","Niski","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Wysoki","m³/min","","29.2","","34.0"]
["","","","Cicha praca","m³/min","","17.6","","22.1"]
["","","Chłodzenie","Cicha praca","m³/min","","17.6","","22.1"]
["Panel dekoracyjny","Ciężar","","","kg","","4","","4"]
["","Wymiary","","Wysokość","mm","","82","","82"]
["","","","Głębokość","mm","","990","","990"]
["","","","Szerokość","mm","","990","","990"]
["","Kolor","","","","","Biały","","Biały"]
["Power supply","Phase","","","","","1~","","1~"]
["","Nazwa","","","","","V1","","V1"]
["","Częstotliwość","","","Hz","","50","","50"]
["","Napięcie","","","V","","220-240","","220-240"]
["Wentylator","Przepływ powietrza","Grzanie","Cicha praca","m³/min","15","","22.1"]
["Pobór mocy","Grzanie","","Nom.","kW","0.067","","0.137"]
["","Chłodzenie","","Nom.","kW","0.067","","0.137"]
["Wentylator","Przepływ powietrza","Chłodzenie","Cicha praca","m³/min","15","","22.1"]
["Obudowa","Materiał","","","","Stal galwanizowana","","Stal galwanizowana"]
["Wymiary","Jednostka","","Wysokość","mm","265","","300"]
["","","","Szerokość","mm","820","","820"]
["","","","Głębokość","mm","820","","820"]
["Ciężar","Jednostka","","","kg","31","","39"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Niski","m³/min","17.6","","26.3"]
["","","Grzanie","Wysoki","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Niski","m³/min","17.6","","26.3"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","54","","60"]
["","Ogrzewanie","","","dBA","54","","60"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Niski","dBA","35","","43"]
["","","","Cicha praca","dBA","32","","41"]
["","Grzanie","","Wysoki","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Niski","dBA","35","","43"]
["","","","Cicha praca","dBA","32","","41"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52","","9.52"]
["","Gaz","","Śr. zewn.","mm","15.88","","15.88"]
["","Spust","","","","19.05","","19.05"]
["Panel dekoracyjny","Wymiary","","Wysokość","mm","82","","82"]
["","","","Szerokość","mm","990","","990"]
["","","","Głębokość","mm","990","","990"]
["","Ciężar","","","kg","4","","4"]
["Syst. kontroli","Pilot na podczerwień","","","","ARCWLA","","ARCWLA"]
["","Pilot przewodowy","","","","ARCWB","","ARCWB"]
["Standardowe akcesoria","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","","50"]
["","Napięcie","","","V","220-240","","220-240"]