{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-A"]
[]
[]
[]
[]
["","","","","ADEA50A2VEB / ARXM50A5V1B","ADEA60A2VEB / ARXM60A5V1B","ADEA71A2VEB / ARXM71A5V1B"]
["Wydajność chłodnicza","Nom.","","kW","5.00","5.7","6.8"]
["","Maks.","","kW","","","6.98"]
["Wydajność grzewcza","Nom.","","kW","5.50","7","7.5"]
["","Maks.","","kW","","","7.66"]
["Wydaj. znam.","EER","","","3.27","3.43","2.95"]
["","COP","","","3.74","3.63","3.49"]
["","Rocz. zużycie ener.","","kWh","765","831","1153"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A","A","C"]
["","","Ogrzewanie","","A","A","B"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A+","A+","A"]
["","Wydajność","Pdesign","kW","5.00","5.7","6.8"]
["","SEER","","","5.65","5.74","5.35"]
["","Roczne zużycie energii","","kWh/rok","310","347","445"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A+","A+","A"]
["","Wydajność","Pdesign","kW","4.40","4.6","6"]
["","SCOP/A","","","4.00","4","3.8"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","3.73","4","4.83"]
["","Roczne zużycie energii","","kWh/rok","1538","1610","2209"]
["Uwagi","","","","","(1) - Patrz oddzielny rysunek zakresu pracy","(1) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m."]
["","","","","","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","","(3) - Nominalne wydajności chłodzenia oparte są na: temp. wewnętrzna: 27°CDB, 19°CWB, temp. zewn.: 35°CDB, równoważna dług. rur: 5 m, różnica poziomów: 0 m.","(3) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(4) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(4) - Dane elektryczne, patrz oddzielny rysunek"]