{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":11,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","37","37","31"]
["","","","Czynnik","dBA","34","34","28"]
["","","","Niski","dBA","29","29","25"]
["","Chłodzenie","","Medium","dBA","32","32","28"]
["","","","Niski","dBA","29","29","25"]
["","","","Wysoki","dBA","35","35","30"]
["Standardowe akcesoria","Instrukcja obsługi","","","","1","1","1"]
["","Instrukcja instalacji","","","","1","1","1"]
["","Przewód spustowy","","","","1","1","1"]
["","Zacisk metalowy na przewodzie spustowym","","","","1","1","1"]
["","Podkładka do wspornika wieszaka","","","","8","8","8"]
["","Śruby","","","","40","40","40"]
["","Izolacja mocowania","","","","2","2","2"]
["","Podkładki uszczelniające","","","","5","5","5"]
["","Zaciski","","","","4","4","4"]
["Syst. kontroli","Wired remote control","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Piping connections","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.52","12.70","12.70"]
["","Spust","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","60","60","56"]
["Wymiary","Jednostka","","Szerokość","mm","700","700","1,000"]
["","","","Głębokość","mm","800","800","800"]
["","","","Wysokość","mm","245","245","245"]
["Obudowa","Materiał","","","","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["","Colour","","","","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)"]
["Ciężar","Jednostka","","","kg","28.0","28.0","35.0"]
["Wentylator","Spręż dyspozycyjny","","Wysoki","Pa","150","150","150"]
["","","","Nom.","Pa","30","30","30"]
["","Przepływ powietrza","Grzanie","Wysoki","m³/min","15.0","15.0","18.0"]
["","","","Niski","m³/min","10.5","10.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0"]
["","","Chłodzenie","Niski","m³/min","10.5","10.5","12.5"]
["","","","Medium","m³/min","12.5","12.5","15.0"]
["","","","Wysoki","m³/min","15.0","15.0","18.0"]
["Wysokość spustu","mm","","","","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Częstotliwość","","","Hz","50","50","50"]
["","Napięcie","","","V","220-240/220","220-240/220","220-240/220"]
["Uwagi","","","","","(1) - Poziom głośności jest wartością bezwzględną generowaną przez źródło dźwięku.","(1) - Poziom głośności jest wartością bezwzględną generowaną przez źródło dźwięku.","(1) - Poziom głośności jest wartością bezwzględną generowaną przez źródło dźwięku.","(1) - Poziom głośności jest wartością bezwzględną generowaną przez źródło dźwięku.","(1) - Poziom głośności jest wartością bezwzględną generowaną przez źródło dźwięku.","(1) - Poziom głośności jest wartością bezwzględną generowaną przez źródło dźwięku."]
["","","","","","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek","(2) - Dane elektryczne, patrz oddzielny rysunek"]
["Wentylator","Spręż dyspozycyjny","","Wysokie","Pa","","","","150","150","150"]
["Obudowa","Kolor","","","","","","","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)","Nie pokryta (galwanizowana)"]
["","Materiał","","","","","","","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["Wymiary","Jednostka","","Wysokość","mm","","","","245","245","245"]
["","","","Szerokość","mm","","","","1000","1400","1400"]
["","","","Głębokość","mm","","","","800","800","800"]
["Ciężar","Jednostka","","","kg","","","","35","46","46"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","","","18","29","34"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","","","15","26","29"]
["","","","Niski","m³/min","","","","12.5","23","23.5"]
["","","Grzanie","Wysoki","m³/min","","","","18","29","34"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","","","","15","26","29"]
["","","Grzanie","Niski","m³/min","","","","12.5","23","23.5"]
["","Spręż dyspozycyjny","","Nom.","Pa","","","","30","40","50"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","","","56","58","62"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","","","30","34","37"]
["","","","Czynnik","dBA","","","","28","32","35"]
["","","","Niski","dBA","","","","25","30","32"]
["","Grzanie","","Wysoki","dBA","","","","31","36","38"]
["","Ogrzewanie","","Czynnik","dBA","","","","28","33","35"]
["","Grzanie","","Niski","dBA","","","","25","30","32"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","","","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","","","","15.9","15.9","15.9"]
["","Spust","","","","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Wysokość spustu","mm","","","","","","","625","625","625"]
["Syst. kontroli","Pilot na podczerwień","","","","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Pilot przewodowy","","","","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardowe akcesoria","Installation manual","","","","","","","1","1","1"]
["","Washer for hanger bracket","","","","","","","8","8","8"]
["","Operation manual","","","","","","","1","1","1"]
["","Clamps","","","","","","","4","4","4"]
["","Drain hose","","","","","","","1","1","1"]
["","Insulation for fitting","","","","","","","2","2","2"]
["","Metal clamp for drain hose","","","","","","","1","1","1"]
["","Screws","","","","","","","40","40","40"]
["","Sealing pads","","","","","","","5","5","5"]
["Zasilanie energią elektryczną","liczba faz","","","","","","","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","","50","50","50"]
["","Napięcie","","","V","","","","220-240/220","220-240/220","220-240/220"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","","","","","","14.00"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","","","","","","13.50"]