{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB (Archived)","ADEQ100C2VEB (Archived)","ADEQ125C2VEB (Archived)"]
["Wentylator","Spręż dyspozycyjny","","Wysokie","Pa","150","150","150","150","150","150"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","","","","","","12.10"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","","","","","","13.5"]
["Obudowa","Kolor","","","","Nie powlekana","Nie powlekana","Nie powlekana","Nie powlekana","Nie powlekana","Nie powlekana"]
["","Materiał","","","","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa","Galwanizowana blacha stalowa"]
["Wymiary","Jednostka","","Wysokość","mm","245","245","245","245","245","245"]
["","","","Szerokość","mm","700","700","1000","1000","1400","1400"]
["","","","Głębokość","mm","800","800","800","800","800","800"]
["Ciężar","Jednostka","","","kg","28","28","35","35","46","46"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","15","15","18","18","29","34"]
["","","","Nom.","m³/min","15.0","15.0","18.0","18.0","29.0","34.0"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","12.5","12.5","15","15","26","29"]
["","","","Niski","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","","Grzanie","Wysoki","m³/min","15","15","18","18","29","34"]
["","","","Nom.","m³/min","15.0","15.0","18.0","18.0","29.0","34.0"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","12.5","12.5","15","15","26","29"]
["","","Grzanie","Niski","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","Spręż dyspozycyjny","","Nom.","Pa","30","30","30","30","40","50"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","60","60","56","56","58","62"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","35","35","30","30","34","37"]
["","","","Nom.","dBA","35","35","30","30","34","37"]
["","","","Czynnik","dBA","32","32","28","28","32","35"]
["","","","Niski","dBA","29","29","25","25","30","32"]
["","Grzanie","","Wysoki","dBA","37","37","31","31","36","38"]
["","Ogrzewanie","","Czynnik","dBA","34","34","28","28","33","35"]
["","Grzanie","","Nom.","dBA","37","37","31","31","36","38"]
["","","","Niski","dBA","29","29","25","25","30","32"]
["Czynnik chłodniczy","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Spust","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1","1","1","1","1"]
["","Podkładka do wspornika wieszaka","","","","8","8","8","8","8","8"]
["","Instrukcja obsługi","","","","1","1","1","1","1","1"]
["","Zaciski","","","","4","4","4","4","4","4"]
["","Przewód spustowy","","","","1","1","1","1","1","1"]
["","Izolacja mocowania","","","","2","2","2","2","2","2"]
["","Zacisk metalowy na przewodzie spustowym","","","","1","1","1","1","1","1"]
["","Śruby","","","","40","40","40","40","40","40"]
["","Podkładka uszczelniająca","","","","5","5","5","5","5","5"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(1) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku."]