{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":12,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-N9"]
[]
[]
[]
[]
["","","","","","ARXM25N2V1B9","ARXM25N5V1B9","ARXM35N5V1B9","ARXM35N2V1B9","ARXM50N2V1B9","ARXM60N2V1B9","ARXM71N2V1B9"]
["Wymiary","Jednostka","","Wysokość","mm","550","550","550","550","734","734","734"]
["","","","Szerokość","mm","765","765","765","765","870","870","870"]
["","","","Głębokość","mm","285","285","285","285","373","373","373"]
["Ciężar","Jednostka","","","kg","32","32","32","32","50","50.0","50.0"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","-10","-10","","-10","-10","-10"]
["","","","Maks.","°CDB","","50","50","","50","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","-21","-21","","-21","-15","-15"]
["","","","Maks.","°CWB","","18","18","","18","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","46","46","49","49","48","48","52"]
["","Grzanie","","Nom.","dBA","47","47","49","49","49","49","52"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Ilość","","","kg","0.76","0.76","0.76","0.76","1.15","1.15","1.15"]
["","Ilość","","","tCO2Eq","0.52","0.52","0.52","0.52","0.78","0.78","0.78"]
["","GWP","","","","675","675","675","675","675","675","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20","20","20","30","30","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,020 (dla długości instalacji rurowej przekraczającej 10 m)","0,035 (dla dług. inst. rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15","15","15","15","20","20","20"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardowe akcesoria","Drain cap","","","","","","","","3","3","3"]
["Sprężarka","Typ","","","","","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]