{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","","49.0"]
["","Chłodzenie","","Nom.","dBA","","49.0"]
["Standardowe akcesoria","Korek spustowy","","","","","1"]
["","Instrukcja instalacji","","","","","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","","1"]
["","Ogólne zalecenia dotyczące bezpieczeństwa","","","","","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Ilość","","","kg","","0.76"]
["","Typ","","","","","R-32"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Maks.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Połączenia instalacji rurowej","Różnica poziomów","IU - OU","Maks.","m","","15"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["Compressor","Type","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","","840"]
["","","","Głębokość","mm","","350"]
["","","","Wysokość","mm","","552"]
["Ciężar","Jednostka","","","kg","","32"]
["Power supply","liczba faz","","","","","1~"]
["","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","220-240"]
["Uwagi","","","","","(1) - Możliwe tylko w połączeniach z  ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Zawiera fluorowane gazy cieplarniane"]
["","","","","","(2) - Możliwe tylko w połączeniach z ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","","(4) - Możliwe tylko w połączeniach z  ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Możliwe tylko w połączeniach z ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Wymiary","Jednostka","","Wysokość","mm","552"]
["","","","Szerokość","mm","840"]
["","","","Głębokość","mm","350"]
["Ciężar","Jednostka","","","kg","32"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (4), 46 (5)"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","46.0"]
["","Grzanie","","Nom.","dBA","47.0"]
["Czynnik chłodniczy","Ilość","","","kg","0.76"]
["","Ilość","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Zasilanie","Częstotliwość","","","Hz","50"]