{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Chłodzenie","","Wysoki","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Standardowe akcesoria","Korek spustowy","","","","","1","1","1","1"]
["","Instrukcja instalacji","","","","","1","1","1","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","","1","1","","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","","1","1","","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Ilość","","","kg","","1.70","1.0","1.2","1.50"]
["","Typ","","","","","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Prędkość obrot.","Chłodzenie","Bardzo niska","obr/min","","","780","780"]
["","","Grzanie","Bardzo niska","obr/min","","","740","740"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Maks.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","10","10","-10"]
["","Grzanie","Temp. otoczenia","Maks.","°CWB","","18","18","18","18"]
["","","","Min.","°CWB","","-15","-15","-15","-15"]
["Piping connections","Różnica poziomów","IU - OU","Maks.","m","","20.0","15","15","20.0"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","65","","","62"]
["","Ogrzewanie","","","dBA","","65","","","62"]
["Sprężarka","Type","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","","825","765","765","825"]
["","","","Głębokość","mm","","300","285","285","300"]
["","","","Wysokość","mm","","735","550","550","735"]
["Ciężar","Jednostka","","","kg","","47","34","34","47"]
["Wentylator","Przepływ powietrza","Grzanie","Bardzo niska","cfm","","","904","904"]
["","","","Bardzo niska","m³/min","","","25.6","25.6"]
["","","Chłodzenie","Bardzo niska","m³/min","","","30.1","30.1"]
["","","","Bardzo niska","cfm","","","1,063","1,063"]
["Power supply","Phase","","","","","1~","1~","1~","1~"]
["","Częstotliwość","","","Hz","","50","50","50","50"]
["","Napięcie","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Uwagi","","","","","(1) - 220 V","","(1) - Po podłączeniu do jednostki zewnętrznej w systemie multi, patrz specyfikacje podłączanej jednostki zewnętrznej multi.","(1) - Po podłączeniu do jednostki zewnętrznej w systemie multi, patrz specyfikacje podłączanej jednostki zewnętrznej multi."]
["","","","","","(2) - 230 V","","(2) - 220 V","(2) - 220 V"]
["","","","","","(3) - 240 V","","(3) - 230 V","(3) - 230 V"]
["","","","","","","","(4) - 240 V","(4) - 240 V"]
["","","","","","","","(5) - Zawiera fluorowane gazy cieplarniane","(5) - Zawiera fluorowane gazy cieplarniane"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","48.9"]
["","","Ogrzewanie","Bardzo niska","m³/min","43.1"]
["","","","Bardzo niska","cfm","1727"]
["","","Ogrzewanie","Bardzo niska","cfm","1522"]
["Wymiary","Jednostka","","Wysokość","mm","735"]
["","","","Szerokość","mm","825"]
["","","","Głębokość","mm","300"]
["Ciężar","Jednostka","","","kg","47"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min","670"]
["","","Ogrzewanie","Bardzo niska","obr/min","670"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","10"]
["","","","Maks.","°CDB","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","48"]
["","Grzanie","","Wysoki","dBA","48"]
["Czynnik chłodniczy","Typ","","","","R-410A"]
["","Ilość","","","kg","1.7"]
["","Ilość","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","20"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]
["Uwagi","","","","","","(1) - Zawiera fluorowane gazy cieplarniane","","","(1) - Zawiera fluorowane gazy cieplarniane"]