{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","48"]
["","","","Niski","dBA","","45"]
["Standardowe akcesoria","1","","","","","550"]
["Czynnik chłodniczy","Charge","","","kg","","2.5"]
["","Typ","","","","","1.2"]
["Wentylator","Przepływ powietrza","Chłodzenie","Bardzo niska","m³/min","","30.1"]
["","","","Bardzo niska","cfm","","1,063"]
["Fan motor","Prędkość","Chłodzenie","Bardzo niska","obr/min_","","740"]
["","","Grzanie","Bardzo niska","obr/min_","","-15"]
["Zakres pracy","Heating","Temp. otoczenia","Min.","°CWB","","20"]
["","","","Maks.","°CWB","","10"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Niski","dBA","","44"]
["","","","Wysoki","dBA","","48"]
["Compressor","Typ","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","","285"]
["","","","Głębokość","mm","","612"]
["","","","Wysokość","mm","","765"]
["Ciężar","Jednostka","","","kg","","34"]
["Wentylator","Przepływ powietrza","Grzanie","Bardzo niska","cfm","","904"]
["","","","Bardzo niska","m³/min","","25.6"]
["Power supply","liczba faz","","","","","1~"]
["","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - Zawiera fluorowane gazy cieplarniane"]
["","","","","","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 230 V"]
["","","","","","","(4) - 240 V"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","30.1"]
["","","Ogrzewanie","Bardzo niska","m³/min","25.6"]
["","","","Bardzo niska","cfm","1063"]
["","","Ogrzewanie","Bardzo niska","cfm","904"]
["Wymiary","Jednostka","","Wysokość","mm","550"]
["","","","Szerokość","mm","765"]
["","","","Głębokość","mm","285"]
["Ciężar","Jednostka","","","kg","34"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","780"]
["","","Ogrzewanie","Bardzo niska","obr/min_","740"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","10"]
["","","","Maks.","°CDB","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","46"]
["","Grzanie","","Wysoki","dBA","47"]
["","","","Niski","dBA","44"]
["Czynnik chłodniczy","Typ","","","","R-410A"]
["","Ilość","","","kg","1.0"]
["","Ilość","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]