{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-J3"]
[]
[]
[]
[]
["","","","","","ATX20J3V1B","ATX25J3V1B","ATX35J3V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.03","0.03","0.030"]
["","Grzanie","","Nom.","kW","0.04","0.04","0.040"]
["Obudowa","Kolor","","","","Biały","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","198","198","198"]
["","","","Szerokość","mm","770","770","770"]
["","","","Głębokość","mm","283","283","283"]
["Ciężar","Jednostka","","","kg","7","7","7.00"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","9.1","9.2","9.3"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","7.4","7.6","7.7"]
["","","","Niski","m³/min","5.9","6","6.1"]
["","","","Cicha praca","m³/min","4.7","4.8","4.9"]
["","","Grzanie","Wysoki","m³/min","9.4","9.7","10.1"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","7.8","8","8.4"]
["","","Grzanie","Niski","m³/min","6.3","6.3","6.7"]
["","","","Cicha praca","m³/min","5.5","5.5","5.7"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","55","55","58"]
["","Ogrzewanie","","","dBA","55","55","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","39","40","41"]
["","","","Czynnik","dBA","33","33","34"]
["","","","Niski","dBA","25","26","27"]
["","","","Cicha praca","dBA","22","22","23"]
["","Grzanie","","Wysoki","dBA","39","40","41"]
["","Ogrzewanie","","Czynnik","dBA","34","34","35"]
["","Grzanie","","Niski","dBA","28","28","29"]
["","","","Cicha praca","dBA","25","25","26"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5","9.50"]
["","Spust","","","","18","18","18"]
["Syst. kontroli","Pilot na podczerwień","","","","ARC433A89","ARC433A89","ARC433A89"]
["Standardowe akcesoria","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1","V1"]
["","liczba faz","","","","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240"]