{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","","","","","43"]
["","","","Czynnik","dBA","","","","","","35"]
["","","","Cicha praca","dBA","","","","","","26"]
["","","","Niski","dBA","","","","","","29"]
["","Chłodzenie","","Medium","dBA","","","","","","34"]
["","","","Cicha praca","dBA","","","","","","20"]
["","","","Niski","dBA","","","","","","27"]
["","","","Wysoki","dBA","","","","","","43"]
["Standardowe akcesoria","Instrukcja instalacji","","","","","","","","","1"]
["","Instrukcja obsługi","","","","","","","","","1"]
["","Zdalny sterownik bezprzewodowy","","","","","","","","","1"]
["","Baterie suche typu AA","","","","","","","","","2"]
["","Uchwyt do pilota","","","","","","","","","1"]
["","Płyta montażowa","","","","","","","","","1"]
["","Tytanowo-apatytowy fotokatalityczny filtr oczyszczający powietrze","","","","","","","","","2"]
["","Śruby mocujące jednostkę wewnętrzną","","","","","","","","","2"]
["Control systems","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","","","","","","6.35"]
["","Gaz","","Śr. zewn.","mm","","","","","","9.50"]
["","Spust","","","","","","","","","18"]
["Power input","Chłodzenie","","Nom.","kW","","","","","","0.024"]
["","Grzanie","","Nom.","kW","","","","","","0.029"]
["Sound power level","Chłodzenie","","","dBA","","","","","","58"]
["","Ogrzewanie","","","dBA","","","","","","58"]
["Wymiary","Jednostka","","Szerokość","mm","","","","","","770"]
["","","","Głębokość","mm","","","","","","225"]
["","","","Wysokość","mm","","","","","","286"]
["Obudowa","Kolor","","","","","","","","","Biały"]
["Ciężar","Jednostka","","","kg","","","","","","9.0"]
["Power supply","liczba faz","","","","","","","","","1~"]
["","Częstotliwość","","","Hz","","","","","","50"]
["","Nazwa","","","","","","","","","V1"]
["","Napięcie","","","V","","","","","","220-240"]
["Uwagi","","","","","","","","","","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Grzanie","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Obudowa","Kolor","","","","Biały","Biały","Biały","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","286","286","286","286","286"]
["","","","Szerokość","mm","770","770","770","770","770"]
["","","","Głębokość","mm","225","225","225","225","225"]
["Ciężar","Jednostka","","","kg","8.5","8.5","8.5","8.5","9"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","7.8","7.8","8","8","8.2"]
["","","","Niski","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Cicha praca","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Grzanie","Wysoki","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","Grzanie","Niski","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Cicha praca","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","55","55","55","55","58"]
["","Ogrzewanie","","","dBA","55","55","55","55","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","39","39","40","40","43"]
["","","","Czynnik","dBA","33","33","33","33","34"]
["","","","Niski","dBA","25","25","26","26","27"]
["","","","Cicha praca","dBA","20","20","20","20","20"]
["","Grzanie","","Wysoki","dBA","39","39","40","40","43"]
["","Ogrzewanie","","Czynnik","dBA","34","34","34","34","35"]
["","Grzanie","","Niski","dBA","28","28","28","28","29"]
["","","","Cicha praca","dBA","23","23","23","23","26"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5","9.5","9.5","9.5"]
["","Spust","","","","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Syst. kontroli","Pilot przewodowy","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1","V1","V1","V1"]
["","liczba faz","","","","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standardowe akcesoria","AAA dry-cell batteries","","","","","2","","2","2"]
["Syst. kontroli","Pilot na podczerwień","","","","","","ARC480A11","ARC480A11"]
["Standardowe akcesoria","Titanium apatite photocatalytic air purification filter","","","","","","2"]