{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Wydajność chłodnicza","Nom.","","kW","","2.50","3.50"]
["Efektywność nominalna","EER","","","","3.79","3.45"]
["","COP","","","","4.36","4.02"]
["","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","","A","A"]
["","","Ogrzewanie","","","A","A"]
["Wydajność grzewcza","Nom.","","kW","","3.00","4.00"]
["Uwagi","","","","","(1) - Chłodzenie: T2: temp. wewn. 26,6°CDB, 19,4°CWB, temp. zewn. 48°CDB [Btu/hr/W]","(1) - Chłodzenie: T2: temp. wewn. 26,6°CDB, 19,4°CWB, temp. zewn. 48°CDB [Btu/hr/W]"]
["","","","","","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m.","(2) - Nominalne wydajności grzewcze oparte są na: temperaturze wewnętrznej: 20°CDB; temperaturze zewnętrznej: 7°CDB, 6°CWB , równorzędnej instalacji chłodniczej: 5 m, różnicy poziomów: 0 m."]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek"]
["Jednostka zewnętrzna","","","","ARXP20K3V1B"]
["Wydajność chłodnicza","Nom.","","kW","2.00"]
["Wydajność grzewcza","Nom.","","kW","2.50"]
["Wydaj. znam.","EER","","","3.98"]
["","COP","","","4.77"]
["Efektywność nominalna","Dyrektywa na temat oznaczeń zużycia energii (klas energetycznych)","Chłodzenie","","A"]
["","","Ogrzewanie","","A"]
["Chłodzenie pomieszczeń","Klasa efektywności energetycznej","","","A++"]
["","Wydajność","Pdesign","kW","2.00"]
["","SEER","","","6.75"]
["","Roczne zużycie energii","","kWh/rok","104"]
["Ogrzewanie pomieszczeń (przeciętny klimat)","Klasa efektywności energetycznej","","","A++"]
["","Wydajność","Pdesign","kW","2.20"]
["","SCOP/A","","","4.64"]
["","Pdh Wydajność grzewcza w temp. -10°","","kW","2.19"]
["","Roczne zużycie energii","","kWh/rok","664"]