{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","12.10"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","13.5"]
["Obudowa","Kolor","","","","Świeży biały"]
["Wymiary","Jednostka","","Wysokość","mm","1850"]
["","","","Szerokość","mm","600"]
["","","","Głębokość","mm","350"]
["Ciężar","Jednostka","","","kg","50"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","28"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","26"]
["","","","Niski","m³/min","24"]
["","","Grzanie","Wysoki","m³/min","28"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","26"]
["","","Grzanie","Niski","m³/min","24"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","63"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","51"]
["","","","Czynnik","dBA","48"]
["","","","Niski","dBA","46"]
["","Grzanie","","Wysoki","dBA","51"]
["","Ogrzewanie","","Czynnik","dBA","46"]
["","Grzanie","","Nom.","dBA","48"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","9.52"]
["","Gaz","","Śr. zewn.","mm","15.9"]
["","Spust","","","","I.D. 20/O.D. 26"]
["Syst. kontroli","Pilot przewodowy","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50/60"]
["","Napięcie","","","V","220-240/220"]