{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BAEF125AWB"]
[]
[]
[]
[]
["","","","","BAEF125AWB."]
["Pobór mocy","kW","","","0.006"]
["Obudowa","Kolor","","","Gray"]
["","LED operacyjne","Kolor","","Blue/red"]
["Wymiary","Jednostka","Wysokość","mm","100"]
["","","Szerokość","mm","840"]
["","","Głębokość","mm","840"]
["","Jednostka zapakowana","Wysokość","mm","168"]
["","","Szerokość","mm","910"]
["","","Głębokość","mm","910"]
["Ciężar","Jednostka","","kg","12.0"]
["","Jednostka zapakowana","","kg","15.5"]
["Opakowanie","Materiał","","","Tektura"]
["","Ciężar","","kg","4"]
["Power supply","liczba faz","","","1~"]
["","Częstotliwość","","Hz","50/60"]
["","Napięcie","","V","220-240/220"]
["Uwagi","","","","(1) - Z 2 czujnikami (współczynnik regulacji 0,65): A+ ; Inne: A"]