{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Zastosowanie","","","","","Typ przypodłogowy"]
["Wydajność","m³/min","","","","33.33"]
["Obudowa","Kolor","","","","Lakierowana blacha stalowa ocynkowana"]
["Wymiary","Jednostka","","Wysokość","mm","1628"]
["","","","Szerokość","mm","720"]
["","","","Głębokość","mm","770"]
["Ciężar","Jednostka","","","kg","150"]
["Zastosowanie do pomieszczeń o powierzchni","m²","","","","133"]
["Oczyszczanie powietrza","Pobór mocy","","H","kW","0.379"]
["Poziom ciśnienia akustycznego","Oczyszczanie powietrza","","Wysoki","dBA","55.9"]
["Wentylator","Przepływ powietrza","Oczyszczanie powietrza","Turbo","m³/h","2300"]
["","","","Wysoki","m³/h","2000"]
["Urządzenia bezpieczeństwa","Pozycja","","01","","Wyłącznik bezpieczeństwa (zatrzymuje pracę urządzenia po otwarciu tylnych drzwi)"]
["Standardowe akcesoria","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Przewód zasilający","m","","","","3"]
["Zasilanie","Częstotliwość","","","Hz","50/60"]
["Prąd roboczy","Oczyszczanie powietrza","","Wysoki","A","1.73"]