{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53C"]
[]
[]
[]
[]
["","","","","BRC1E53C7"]
["Opakowanie","Materiał","","","Karton_"]
["","Ciężar","","kg","0.05"]
["Temperatura otoczenia","Wilgotność względna <","","%","95"]
["Wymiary","Jednostka zapakowana","Szerokość","mm","160"]
["","","Wysokość","mm","55"]
["","","Głębokość","mm","150"]
["","Jednostka","Szerokość","mm","120"]
["","","Głębokość","mm","19"]
["","","Wysokość","mm","120"]
["Obudowa","Osłona przycisku","","","Nie"]
["","Colour","","","Świeży biały"]
["","LED operacyjne","Kolor","","Zielony"]
["LCD","Typ","","","W całości punktowa (160 x 255)"]
["","Podświetlenie","Kolor","","Biały"]
["","Wymiary","Szerokość","mm","68.85"]
["","","Wysokość","mm","43.2"]
["Ciężar","Jednostka zapakowana","","kg","0.415"]
["","Jednostka","","kg","0.200"]
["Back-up for power failure","","","","Tak (zegar będzie działał przez okres nie przekraczający 48 godzin)"]
["Złącza przewodów","Długość okablowania","Maks.","m","500"]