{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDK"]
[]
[]
[]
[]
["","","","","BRC1HHDAK (Archived)","BRC1HHDAKA (Archived)"]
["Obudowa","Kolor","","","Czarny","Czarny"]
["","Osłona przycisku","","","Nie","Nie"]
["","LED operacyjne","Kolor","","Niebieski wskaźnik statusu","Niebieski wskaźnik statusu"]
["Wymiary","Jednostka","Wysokość","mm","85","85"]
["","","Szerokość","mm","85","85"]
["","","Głębokość","mm","25","25"]
["","Jednostka zapakowana","Wysokość","mm","50","50"]
["","","Szerokość","mm","217","217"]
["","","Głębokość","mm","161","161"]
["Ciężar","Jednostka","","kg","0.110","0.110"]
["","Jednostka zapakowana","","kg","0.317","0.317"]
["Opakowanie","Materiał","","","Tektura","Tektura"]
["","Ciężar","","kg","0.0850","0.0850"]
["LCD","Typ","","","100 x 150 punktów","100 x 150 punktów"]
["","Wymiary","Wysokość","mm","40.7","40.7"]
["","","Szerokość","mm","28.0","28.0"]
["","Podświetlenie","Kolor","","Biały","Biały"]
["Temp. otoczenia","Działanie","Min.","°C","-10","-10"]
["","","Maks.","°C","50","50"]
["","Przechowywanie","Min.","°C","-20","-20"]
["","","Maks.","°C","70","70"]
["","Temp. otoczenia-=-Wilgotność względna <-=-%","","%","95","95"]
["Systemy sterujące","Klasa sterownika temperatury","","","VI","VI"]
["","Wkład do sezonowej efektywności ogrzewania pomieszczeń","","%","4.0","4.0"]
["Złącza przewodów","Długość okablowania","Maks.","m","500","500"]