{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-A"]
[]
[]
[]
[]
["","","","","","CHYHBH05AFV32 / 3MXM52A2V1B","CHYHBH05AAV32 / 3MXM52A2V1B","CHYHBH05AFV32 / 3MXM68A2V1B","CHYHBH05AAV32 / 3MXM68A2V1B"]
["Podgrzewanie ciepłej wody użytkowej","Informacje ogólne","","Zadeklarowany profil obciążenia","","XL","","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","A","","A"]
["COP","","","","","4.49 (1)","4.49 (1)","3.91 (1)","3.91 (1)"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Seasonal space heating eff. class","","A+","","A+"]
["","","","ηs (sprawność sezonowa ogrzewania pomieszczeń)","%","111.4","","113.3"]
["","","","SCOP","","2.86","","2.91"]
["Wydajność grzewcza","Nom.","","","kW","4.41 (1)","","4.50 (1)"]
["Uwagi","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła"]
["Wydajność grzewcza","Nom.","","","kW","","4.41 (1)","","4.5 (1)"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","","XL","","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","","A","","A"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","","2.86","","2.91"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","A+","","A+"]