{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":11,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 4MXM-N"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 4MXM68N2V1B","CHYHBH05AAV32 / 4MXM80N2V1B","CHYHBH08AAV32 / 4MXM80N2V1B","CHYHBH05AFV32 / 4MXM68N2V1B","CHYHBH05AFV32 / 4MXM80N2V1B","CHYHBH08AFV32 / 4MXM80N2V1B"]
["Podgrzewanie ciepłej wody użytkowej","Ogólny","","Zadeklarowany profil obciążenia","","XL","XL","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","A","A","A"]
["COP","","","","","3.91 (1)","4.04 (1)","4.17 (1)","3.91","4.04","4.17"]
["Ogrzewanie pomieszczeń","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Seasonal space heating eff. class","","A+","A+","A+"]
["","","","ηs (sprawność sezonowa ogrzewania pomieszczeń)","%","113.3","120.8","120.8"]
["","","","SCOP","","2.91","3.09","3.09"]
["Wydajność grzewcza","Nom.","","","kW","4.50 (1)","4.50 (1)","6.78 (1)"]
["Uwagi","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła"]
["Wydajność grzewcza","Nom.","","","kW","","","","4.5","4.5","6.78"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","","","","XL","XL","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","","","","A","A","A"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","","","","2.91","3.09","3.09"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","","","A+","A+","A+"]
["Zakres efektywności energetycznej","","","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]