{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AW"]
[]
[]
[]
[]
["","","","","","CTXA15A2V1BW"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","39"]
["","","","Czynnik","dBA","32"]
["","","","Cicha praca","dBA","21"]
["","","","Niski","dBA","25"]
["","Chłodzenie","","Medium","dBA","32"]
["","","","Cicha praca","dBA","21"]
["","","","Niski","dBA","25"]
["","","","Wysoki","dBA","39"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1"]
["","Instrukcja obsługi","","","","1"]
["","Filtr powietrza","","","","2"]
["","Zdalny sterownik bezprzewodowy","","","","1"]
["","Zdalny element sterujący płytą montażową","","","","1"]
["","Torebka ze śrubami","","","","1"]
["","Pokrywa na śruby","","","","1"]
["","Baterie suche typu AAA","","","","2"]
["","Ogólne zalecenia dotyczące bezpieczeństwa","","","","1"]
["Czynnik chłodniczy","GWP","","","","675.0"]
["Control systems","Wired remote control","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35"]
["","Gaz","","Śr. zewn.","mm","9.50"]
["","Spust","","","","18"]
["Power input","Chłodzenie","","Nom.","kW","0.020"]
["","Grzanie","","Nom.","kW","0.020"]
["Sound power level","Chłodzenie","","","dBA","57"]
["Wymiary","Jednostka","","Szerokość","mm","798"]
["","","","Głębokość","mm","189"]
["","","","Wysokość","mm","295"]
["Obudowa","Kolor","","","","Biały"]
["Ciężar","Jednostka","","","kg","12"]
["Wentylator","Natężenie przepływu powietrza","Grzanie","Wysoki","m³/min","10.9"]
["","","","Medium","m³/min","8.7"]
["","","","Niski","m³/min","6.4"]
["","","","Cicha praca","m³/min","4.5"]
["","","Chłodzenie","Niski","m³/min","6.1"]
["","","","Medium","m³/min","8"]
["","","","Wysoki","m³/min","11.0"]
["","","","Cicha praca","m³/min","4.6"]
["Power supply","liczba faz","","","","1~"]
["","Nazwa","","","","V1"]
["","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]