{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXF-C"]
[]
[]
[]
[]
["","","","","","CTXF20C5V1B","CTXF25C5V1B","CTXF35C5V1B"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.017","0.019","0.032"]
["","Grzanie","","Nom.","kW","0.02","0.02","0.032"]
["Obudowa","Kolor","","","","Biały","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","286","286","286"]
["","","","Szerokość","mm","770","770","770"]
["","","","Głębokość","mm","225","225","225"]
["Ciężar","Jednostka","","","kg","8.5","8","9"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","9.8","10.1","11.5"]
["Wentylator","Przepływ powietrza","Chłodzenie","Czynnik","m³/min","8","8","8"]
["Wentylator","Przepływ powietrza","Chłodzenie","Niski","m³/min","5.9","6.1","6.3"]
["","","","Cicha praca","m³/min","4.4","4.4","4.5"]
["","","Grzanie","Wysoki","m³/min","10.3","10.3","11.5"]
["Wentylator","Przepływ powietrza","Grzanie","Czynnik","m³/min","8.4","8.6","9"]
["Wentylator","Przepływ powietrza","Grzanie","Niski","m³/min","6.5","6.7","7"]
["","","","Cicha praca","m³/min","5.3","5.3","5.3"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","55","55","58"]
["","Ogrzewanie","","","dBA","55","55","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","39","40","43"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Czynnik","dBA","33","33","34"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Niski","dBA","25","26","27"]
["","","","Cicha praca","dBA","20","20","20"]
["","Grzanie","","Wysoki","dBA","39","40","40"]
["","Ogrzewanie","","Czynnik","dBA","34","34","35"]
["","Grzanie","","Niski","dBA","28","28","29"]
["","","","Cicha praca","dBA","21","21","21"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35","6.35"]
["Połączenia instalacji rurowej","Gaz","","Śr. zewn.","mm","9.5","9.5","9.5"]
["Połączenia instalacji rurowej","Spust","","","","18","18","18"]
["Syst. kontroli","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Pilot przewodowy","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardowe akcesoria","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Batteries","","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~"]
["Zasilanie","Zasilanie-=-Częstotliwość","","Częstotliwość","","50","50","50"]
["","Zasilanie-=-Napięcie","","Napięcie","","220-440","220-440","220-440"]