{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B (Archived)","CTXM15R5V1B (Archived)"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.029","0.029"]
["","Grzanie","","Nom.","kW","0.023","0.023"]
["Obudowa","Kolor","","","","Biały","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","295","295"]
["","","","Szerokość","mm","778","778"]
["","","","Głębokość","mm","272","272"]
["Ciężar","Jednostka","","","kg","10","10"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","10.5","10.5"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","7.5","7.5"]
["","","","Niski","m³/min","5.7","5.7"]
["","","","Cicha praca","m³/min","4.3","4.3"]
["","","Grzanie","Wysoki","m³/min","9.3","9.3"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","8.2","8.2"]
["","","Grzanie","Niski","m³/min","6.2","6.2"]
["","","","Cicha praca","m³/min","5.1","5.1"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","57","57"]
["","Ogrzewanie","","","dBA","54","54"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","41","41"]
["","","","Czynnik","dBA","33","33"]
["","","","Niski","dBA","25","25"]
["","","","Cicha praca","dBA","19","19"]
["","Grzanie","","Wysoki","dBA","39","39"]
["","Ogrzewanie","","Czynnik","dBA","34","34"]
["","Grzanie","","Niski","dBA","26","26"]
["","","","Cicha praca","dBA","20","20"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","9.5"]
["","Spust","","","","18","18"]
["Syst. kontroli","Pilot na podczerwień","","","","ARC466A67","ARC466A67"]
["","Pilot przewodowy","","","","BRC073A1","BRC073A1"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1"]
["","Pilot bezprzewodowy","","","","1","1"]
["","Baterie suche typu AAA","","","","2","2"]
["","Zestaw adaptera WLAN","","","","1","1"]
["","Instrukcja obsługi","","","","1","1"]
["","Tytanowo-apatytowy filtr eliminujący zapachy","","","","1","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","","2","2"]
["","Płyta montażowa","","","","1","1"]
["","Uchwyt do pilota","","","","1","1"]
["Zakres efektywności energetycznej","","","","","A+++ ~ D","A+++ ~ D"]
["Zasilanie energią elektryczną","Nazwa","","","","V1","V1"]
["","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m","(1) - Chłodzenie: temp. wewn. 27°CDB, 19,0°CWB; temp. zewnętrznej 35°CDB, 24°CWB; długość równoważna instalacji rurowej: 5 m"]
["","","","","","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m","(2) - Grzanie: temp. wewn. 20°CDB; temp. zewnętrzna 7°CDB, 6°CWB , równoważna instalacja chłodnicza: 5 m"]