{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","38","","41"]
["","","","Cicha praca","dBA","21","","21"]
["","","","Niski","dBA","28","","30"]
["","Chłodzenie","","Cicha praca","dBA","21","","21"]
["","","","Niski","dBA","25","","28"]
["","","","Wysoki","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Chłodzenie","","Nom.","dBA","31","","35"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","","1"]
["","Instrukcja obsługi","","","","1","","1"]
["","Pilot bezprzewodowy","","","","1","","1"]
["","Baterie","","","","2","","2"]
["","Uchwyt do pilota","","","","1","","1"]
["","Płyta montażowa","","","","1","","1"]
["","Śruby mocujące jednostkę wewnętrzną","","","","2","","2"]
["","Tytanowo-apatytowy fotokatalityczny filtr oczyszczający powietrze","","","","2","","2"]
["Syst. kontroli","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.35","","6.35"]
["","Gaz","","Śr. zewn.","mm","9.5","","9.5"]
["","Spust","","","","18","","18"]
["Power input","Chłodzenie","","Nom.","kW","0.040","","0.040"]
["","Grzanie","","Nom.","kW","0.040","","0.040"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","55","","59"]
["","Ogrzewanie","","","dBA","56","","58"]
["Wymiary","Jednostka","","Szerokość","mm","780","","780"]
["","","","Głębokość","mm","215","","215"]
["","","","Wysokość","mm","289","","289"]
["Obudowa","Kolor","","","","Biały","","Biały"]
["Ciężar","Jednostka","","","kg","8","","8"]
["Wentylator","Natężenie przepływu powietrza","Ogrzewanie","Wysoki","m³/min","","","10.1"]
["","","","Niski","m³/min","","","6.3"]
["","","","Cicha praca","m³/min","","","4.3"]
["","","Chłodzenie","Niski","m³/min","","","5.2"]
["","","","Wysoki","m³/min","","","9.2"]
["","","","Cicha praca","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Chłodzenie","Nom.","m³/min","","","7.2"]
["Power supply","liczba faz","","","","1~","","1~"]
["","Częstotliwość","","","Hz","50","","50"]
["","Nazwa","","","","V1","","V1"]
["","Napięcie","","","V","220-240","","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Pobór mocy","Chłodzenie","","Nom.","kW","","0.04","","0.040"]
["","Grzanie","","Nom.","kW","","0.04","","0.040"]
["Obudowa","Kolor","","","","","Biały","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","","289","","289"]
["","","","Szerokość","mm","","780","","780"]
["","","","Głębokość","mm","","215","","215"]
["Ciężar","Jednostka","","","kg","","8","","8.00"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","","7.9","","9.2"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","","6.3","","7.2"]
["","","","Niski","m³/min","","4.7","","5.2"]
["","","","Cicha praca","m³/min","","3.9","","3.9"]
["","","Grzanie","Wysoki","m³/min","","9","","10.1"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","","7.5","","8.1"]
["","","Grzanie","Niski","m³/min","","6","","6.3"]
["","","","Cicha praca","m³/min","","4.3","","4.3"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","55","","59"]
["","Ogrzewanie","","","dBA","","56","","58"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","37","","42"]
["","","","Czynnik","dBA","","31","","35"]
["","","","Niski","dBA","","25","","28"]
["","","","Cicha praca","dBA","","21","","21"]
["","Grzanie","","Wysoki","dBA","","38","","41"]
["","Ogrzewanie","","Czynnik","dBA","","33","","36"]
["","Grzanie","","Niski","dBA","","28","","30"]
["","","","Cicha praca","dBA","","21","","21"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","6.35","","6.35"]
["","Gaz","","Śr. zewn.","mm","","9.5","","9.50"]
["","Spust","","","","","18","","18"]
["Syst. kontroli","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standardowe akcesoria","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Zasilanie energią elektryczną","Nazwa","","","","","V1","","V1"]
["","liczba faz","","","","","1~","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50","","50"]
["","Napięcie","","","V","","220-240","","220-240"]