{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Pobór mocy","Chłodzenie","","Nom.","kW","0.02"]
["","Grzanie","","Nom.","kW","0.02"]
["Obudowa","Kolor","","","","Biały"]
["Wymiary","Jednostka","","Wysokość","mm","600"]
["","","","Szerokość","mm","750"]
["","","","Głębokość","mm","238"]
["Ciężar","Jednostka","","","kg","17"]
["Wentylator","Przepływ powietrza","Chłodzenie","Wysoki","m³/min","8.7"]
["","Natężenie przepływu powietrza","Chłodzenie","Czynnik","m³/min","7"]
["","","","Niski","m³/min","4.9"]
["","","","Cicha praca","m³/min","4.1"]
["","","Grzanie","Wysoki","m³/min","9.2"]
["","Natężenie przepływu powietrza","Ogrzewanie","Czynnik","m³/min","7.2"]
["","","Grzanie","Niski","m³/min","5.6"]
["","","","Cicha praca","m³/min","4.1"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","52"]
["","Ogrzewanie","","","dBA","52"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","38"]
["","","","Czynnik","dBA","32"]
["","","","Niski","dBA","25"]
["","","","Cicha praca","dBA","22"]
["","Grzanie","","Wysoki","dBA","38"]
["","Ogrzewanie","","Czynnik","dBA","32"]
["","Grzanie","","Niski","dBA","25"]
["","","","Cicha praca","dBA","21"]
["Czynnik chłodniczy","GWP","","","","675"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","6.4"]
["","Gaz","","Śr. zewn.","mm","9.5"]
["","Spust","","","","VP20 (I.D. 20/O.D. 26)"]
["Syst. kontroli","Infrared remote control","","","","ARC466A66"]
["Syst. kontroli","Pilot przewodowy","","","","BRC073A1"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]