{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Pobór mocy","kW","","","","0.015"]
["Maks. liczba możliwych do podłączenia jedn. wewnętrznych","","","","","32"]
["Maks. liczba możliwych do podłączenia jedn. zewnętrznych @","","","","","7"]
["Wymiary","Jednostka","","Wysokość","mm","136"]
["","","","Szerokość","mm","384"]
["","","","Głębokość","mm","92"]
["Komunikacja","DIII-NET","","Ilość","","1"]
["","","","Uwaga","","DIII-NET (F1F2)"]
["","Ethernet","","Ilość","","1"]
["","Terminal wejściowy","Cyfrowy","Ilość","","4"]
["Temp. otoczenia","Działanie","","Min.","°C","-10"]
["","","","Maks.","°C","50"]
["","Przechowywanie","","Min.","°C","-20"]
["","","","Maks.","°C","60"]
["","Temp. otoczenia-=-Wilgotność względna <-=-%","","","%","85"]
["Zasilanie","Częstotliwość","","","Hz","50/60"]
["","Napięcie","","","V","prąd przemienny 110-240 V"]
["Uwagi","","","","","(1) - Obejmuje zasilanie z zasilacza WAGO, moduł CPU (procesora) oraz moduł I/O (wejść/wyjść)"]
["","","","","","(2) - Wymiary obejmują zasilacz WAGO, moduł CPU, moduł I/O oraz niezbędne odstępy pomiędzy poszczególnymi częściami"]
["","","","","","(3) - Oto wymiary opcjonalnego ekranu: wysokość: 209 mm, szerokość: 123 mm, grubość: 8,5 mm"]