{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Wejście","Typ","","","","Panel dotykowy (10 bit, kodowane wejście analogowe)"]
["Temperatura otoczenia","Wilgotność względna <","","","%","85"]
["","Działanie","","Min.","°C","0"]
["","","","Maks.","°C","40"]
["Maks. liczba możliwych do podłączenia jedn. wewnętrznych","","","","","64, 128 (1)"]
["Komunikacja","DIII-NET","","Ilość","","1"]
["","","","Uwaga","","Linia komunikacyjna wyposażenia klimatyzacyjnego"]
["","10BASE-T","","Uwaga","","Opcja z Internetem"]
["","Ethernet","","Uwaga","","Port dostępu do sieci i funkcja poczty e-mail"]
["","Terminal wejściowy","Cyfrowy","Ilość","","1"]
["","","","Uwaga","","Wymuszone wyłączenie"]
["","","Impuls","Ilość","","3"]
["","","","Uwaga","","Impuls pomiaru mocy"]
["","Modem","","Uwaga","","Możliwość zainstalowania modemu na płycie"]
["","PCMCIA","","Uwaga","","Karta pamięci Flash"]
["","RS-232C","","Uwaga","","Adaptor DIII-NET PLUS"]
["Wymiary","Jednostka","","Szerokość","mm","230"]
["","","","Głębokość","mm","107"]
["","","","Wysokość","mm","147"]
["LCD","Typ","","","","QVGA (320 x 240), 4 096 kolorów"]
["","Wymiary","","Szerokość","cale","5.7"]
["Maks. liczba możliwych do podłączenia jedn. zewnętrznych","","","","","10, 20 (1)"]
["Power supply","Częstotliwość","","","Hz","50/60"]
["","Napięcie","","","V","100-240 (dostarczane zewnętrznie)"]
["Uwagi","","","","","(1) - Połączenie z DCS601A51"]