{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Comfort"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Comfort 325","DucoBox Energy Comfort D400"]
["Numer artykułu","","","","","00004485","00004707"]
["Pobór mocy - 50 Hz","Tryb wymiany ciepła","Nom.","Ultra wysoki","kW","0.131 (1)"]
["","Tryb obejściowy","Nom.","Ultra wysoki","kW","0.131 (1)"]
["Obudowa","Materiał","","","","Blacha stalowa z powłoką metaliczną + powłoka galwaniczna","Blacha stalowa z powłoką metaliczną + powłoka galwaniczna"]
["Wymiary","Jednostka","","Wysokość","mm","705","800"]
["","","","Szerokość","mm","700","756"]
["","","","Głębokość","mm","525","583"]
["Ciężar","Jednostka","","","kg","21","47"]
["Wentylator","Szybkość natężenia przepływu powietrza - 50 Hz","Tryb wymiany ciepła","Ultra wysoki","m³/h","325","400"]
["","","Tryb obejściowy","Ultra wysoki","m³/h","325","400"]
["","Spręż dyspozycyjny - 50Hz","","Ultra wysoki","Pa","100"]
["Zakres pracy","Jednostka w pobliżu","","","°CDB","-5°C~40°CDB, wilgotność względna 90% lub mniej"]
["Poziom ciśnienia akustycznego - 50 Hz","Tryb wymiany ciepła","","Ultra wysoki","dBA","63"]
["","Tryb obejściowy","","Ultra wysoki","dBA","63"]
["System wymiany ciepła","","","","","Wymiennik ciepła jawnego z przepływem krzyżowym powietrze-powietrze.","Wymiennik ciepła jawnego z przepływem krzyżowym powietrze-powietrze."]
["Element wymiany ciepła","","","","","PET/Polistyren","v1: PP - v2: PET/Alu (polietylen/aluminium)"]
["Średnica przewodu łączącego","mm","","","","Średnica wewnętrzna Ø160","180"]
["Tryb operacyjny","","","","","Tryb wymiany ciepła, Tryb obejściowy, Tryb ochrony przed szronem","Tryb wymiany ciepła, Tryb obejściowy, Tryb ochrony przed szronem"]
["Klasa SEC","","","","","A+","Patrz Uwaga 2"]
["Maksymalne natężenie przepływu przy sprężu dyspozycyjnym (ESP) 100 Pa","Natężenie przepływu","","","m³/h","325","400"]
["Poziom mocy akustycznej (Lwa)","dB","","","","55","55"]
["Roczne zużycie energii elektrycznej","kWh/rok","","","","117.3","231.7 (1)"]
["Roczna oszczędność na ogrzewaniu","Przeciętny klimat","","","kWh/rok","4714","4515 (1)"]
["","Zimny klimat","","","kWh/rok","9222","8833 (1)"]
["","Ciepły klimat","","","kWh/rok","2132","2042 (1)"]
["Zasilanie energią elektryczną","liczba faz","","","","Układ jednofazowy z uziemieniem","3-core power cable with earthed plug"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","230","230"]
["Uwagi","","","","","(1) - Przy maks. przepływie","(1) - Ręczne sterowanie (bez DCV)"]
["","","","","","(2) - przy 250 m3/h","(2) - Z 2 czujnikami (współczynnik regulacji 0,65): A+ ; Inne: A"]
["","","","","","(3) - przy 100 m3/h","(3) - Filtr powietrza nawiewanego z przepływem dynamicznym (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65% (= G4) Opcja: ISO 16890 ePM1 55% (=F7) Filtr powietrza wywiewanego z przepływem dynamicznym (520 x 190 x 15 mm) Standard: ISO 16890 Coarse 65% (= G4)"]
["","","","","","(4) - przy 325 m3/h"]
["","","","","","(5) - przy 332 m3/h"]
["","","","","","(6) - przy 401 m3/h"]