{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":13,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSX-D / ERLA-DV37"]
[]
[]
[]
[]
["","","","","","EBSX16P30DF / ERLA16D2V37","EBSX16P50DF / ERLA16D2V37","EBSX16P30DF / ERLA16DAV37","EBSX16P50DF / ERLA16DAV37","EBSX16P50DG / ERLA16D2V37","EBSX16P30DG / ERLA16DAV37","EBSX16P30DG / ERLA16D2V37","EBSX16P50DG / ERLA16DAV37"]
["Indoor unit","","","","","EBSX16P30DF","EBSX16P50DF","EBSX16P30DF","EBSX16P50DF","EBSX16P50DG","EBSX16P30DG","EBSX16P30DG","EBSX16P50DG"]
["Wydajność grzewcza","Nom.","","","kW","16.0 (1)","16.0 (1)","16.0 (1)","16.0 (1)","16.0","16.0","16.0","16.0"]
["Wydajność chłodnicza","Nom.","","","kW","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)","13.6 (2)"]
["Pobór mocy","Grzanie","","Nom.","kW","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)","3.53 (1)"]
["","Chłodzenie","","Nom.","kW","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)","4.68 (2)"]
["COP","","","","","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)","4.53 (1)"]
["EER","","","","","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)","2.91 (2)"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","L","XL","L","XL","XL","L","L","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","3.35","3.35","3.35","3.35","3.35","3.35","3.35","3.35"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A++","A++","A++","A++","A++","A++","A++","A++"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 35°C","Informacje ogólne","SCOP","","4.68","4.68","4.68","4.68","4.68","4.68","4.68","4.68"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Uwagi","","","","","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]