{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":21,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSX-D / ERLA11-14DV3"]
[]
[]
[]
[]
["","","","","","EBSX11P30DF / ERLA11D2V3","EBSX11P50DF / ERLA11D2V3","EBSX11P30DF / ERLA11DAV3","EBSX11P50DF / ERLA11DAV3","EBSX11P50DG / ERLA11D2V3","EBSX11P30DG / ERLA11DAV3","EBSX11P30DG / ERLA11D2V3","EBSX11P50DG / ERLA11DAV3","EBSX16P30DF / ERLA14D2V3","EBSX16P50DF / ERLA14D2V3","EBSX16P30DF / ERLA14DAV3","EBSX16P50DF / ERLA14DAV3","EBSX16P50DG / ERLA14D2V3","EBSX16P30DG / ERLA14DAV3","EBSX16P30DG / ERLA14D2V3","EBSX16P50DG / ERLA14DAV3"]
["Jednostka wewnętrzna","","","","","EBSX11P30DF","EBSX11P50DF","EBSX11P30DF","EBSX11P50DF","EBSX11P50DG","EBSX11P30DG","EBSX11P30DG","EBSX11P50DG","EBSX16P30DF","EBSX16P50DF","EBSX16P30DF","EBSX16P50DF","EBSX16P50DG","EBSX16P30DG","EBSX16P30DG","EBSX16P50DG"]
["Wydajność grzewcza","Nom.","","","kW","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","10.6 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0 (1)","12.0","12.0","12.0","12.0"]
["Wydajność chłodnicza","Nom.","","","kW","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","11.2 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)","12.9 (2)"]
["Pobór mocy","Grzanie","","Nom.","kW","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.19 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)","2.46 (1)"]
["","Chłodzenie","","Nom.","kW","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","3.47 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)","4.34 (2)"]
["COP","","","","","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.83 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)","4.87 (1)"]
["EER","","","","","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","3.22 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)","2.98 (2)"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","L","XL","L","XL","XL","L","L","XL","L","XL","L","XL","XL","L","L","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","3.27","3.27","3.27","3.27","3.27","3.27","3.27","3.27","3.26","3.26","3.26","3.26","3.26","3.26","3.26","3.26"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 35°C","Informacje ogólne","SCOP","","4.72","4.72","4.72","4.72","4.72","4.72","4.72","4.72","4.68","4.68","4.68","4.68","4.68","4.68","4.68","4.68"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Uwagi","","","","","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]