{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA09-14DV3"]
[]
[]
[]
[]
["","","","","","EDLA11DAV3","EDLA14DAV3"]
["Wydajność grzewcza","Nom.","","","kW","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)"]
["Pobór mocy","Grzanie","","Nom.","kW","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)"]
["Wymiary","Jednostka","","Wysokość","mm","870","870"]
["","","","Szerokość","mm","1380","1380"]
["","","","Głębokość","mm","460","460"]
["Ciężar","Jednostka","","","kg","147","147"]
["Wentylator","Przepływ powietrza","Grzanie","Wysoki","m³/min","55.8","70.4"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","9 (6)","9 (6)"]
["","","","Maks.","°C","60 (6)","60 (6)"]
["","Ciepła woda użytkowa","Temp. otoczenia","Min.","°CDB","-25","-25"]
["","","","Maks.","°CDB","35","35"]
["","","Strona wodna","Min.","°C","25","25"]
["","","","Maks.","°C","55 (6)","55 (6)"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32"]
["","GWP","","","","675","675"]
["","Ilość","","","kg","3.80","3.80"]
["","Ilość","","","tCO2Eq","2.57","2.57"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","3.32","3.37"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A++","A++"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 35°C","Informacje ogólne","SCOP","","4.64","4.62"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A+++","A+++"]
["Element sprężarki","Główne zasilanie","","Faza","","1~","1~"]
["","","","Napięcie","V","230","230"]
["Zasilanie energią elektryczną","Nazwa","","","","V3","V3"]
["","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","230","230"]
["Uwagi","","","","","(1) - Warunek: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Warunek: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Warunek: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Więcej szczegółów widać na rysunku zakresu pracy","(3) - Więcej szczegółów widać na rysunku zakresu pracy"]
["","","","","","(4) - Zależy od trybu pracy, patrz podręcznik instalacji.","(4) - Zależy od trybu pracy, patrz podręcznik instalacji."]