{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9WG"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9WG","EGSAX10DA9WG"]
["Wydajność grzewcza","Min.","","","kW","0.85"]
["","Nom.","","","kW","3.35"]
["","Maks.","","","kW","7.98"]
["Power input","Nom.","","","kW","0.74"]
["COP","","","","","4.51"]
["Obudowa","Kolor","","","","Szary + Czarny"]
["Wymiary","Jednostka","","Wysokość","mm","1,891"]
["","","","Szerokość","mm","597"]
["","","","Głębokość","mm","666"]
["Ciężar","Jednostka","","","kg","222"]
["Zbiornik","Objętość wody","","","l","180"]
["","Izolacja","","Straty ciepła","kWh/24h","1.2"]
["","Zabezpieczenie przed korozją","","","","Trawienie"]
["Czynnik chłodniczy","Typ","","","","R-32"]
["","GWP","","","","675.0"]
["","Charge","","","kg","1.70"]
["Zakres pracy","Przestrzeń instalacji","","Min.","°C","5"]
["","","","Maks.","°C","35"]
["","Strona solanki","","Min.","°C","-10"]
["","","","Maks.","°C","30"]
["","Heating","Strona wodna","Min.","°C","5"]
["","","","Maks.","°C","65"]
["","Ciepła woda użytkowa","Strona wodna","Min.","°C","25"]
["","","","Maks.","°C","60"]
["Ogrzewanie pomieszczeń","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","SCOP","","3.77 (1)"]
["","","","Seasonal space heating eff. class","","A++"]
["","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","SCOP","","5.18 (1)"]
["","","","Klasa efektywności sezon. ogrzewania pomieszczeń","","A+++"]
["Power supply","liczba faz","","","","1~/3~"]
["","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","230/400"]
["Prąd","zalecane bezpieczniki","","","A","16/32"]
["Uwagi","","","","","(1) - Zgodnie z normami EN14825 i EN14511:2018"]
["","","","","","(2) - Patrz rysunek zakresu działania: zwiększanie zakresu za pomocą wspomagającego elementu grzewczego lub dodatkowego elementu grzejnego"]
["Wydajność grzewcza","Min.","","","kW","","0.85"]
["","Nom.","","","kW","","5.49"]
["","Maks.","","","kW","","9.55"]
["Pobór mocy","Nom.","","","kW","","1.17"]
["COP","","","","","","4.7"]
["Obudowa","Kolor","","","","","SZARY +CZARNY"]
["Wymiary","Jednostka","","Wysokość","mm","","1891"]
["","","","Szerokość","mm","","597"]
["","","","Głębokość","mm","","666"]
["Ciężar","Jednostka","","","kg","","222"]
["Zbiornik","Izolacja","","Straty ciepła","kWh/24h","","1.2"]
["","Zabezpieczenie przed korozją","","","","","Trawienie"]
["Czynnik chłodniczy","Typ","","","","","R-32"]
["","GWP","","","","","675.0"]
["","Ilość","","","tCO2Eq","","1.15"]
["","Ilość","","","kg","","1.70"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","","4.05 (1)"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","A+++"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 35°C","Informacje ogólne","SCOP","","","5.20 (1)"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","A+++"]
["Zasilanie energią elektryczną","liczba faz","","","","","1~/3~"]
["Zasilanie","Częstotliwość","","","Hz","","50"]
["","Napięcie","","","V","","230/400"]
["Prąd","zalecane bezpieczniki","","","A","","16/32"]
["Uwagi","","","","","","(1) - Zgodnie z normami EN14825 i EN14511:2018"]