{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Poziom ciśnienia akustycznego","Nom.","","","dBA","32.0 (6)"]
["Czynnik chłodniczy","GWP","","","","2,090"]
["","Dopełnienie","","","kg","1.80"]
["","Typ","","","","R-410A"]
["Zakres pracy","Przestrzeń instalacji","","Min.","°C","5.00"]
["","","","Maks.","°C","30.0"]
["","Ogrzewanie","Strona wodna","Maks.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Strona solanki","","Min.","°C","-5.00"]
["","","","Maks.","°C","20.0"]
["","Ciepła woda użytkowa","Strona wodna","Maks.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Power input","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Poziom mocy akustycznej","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Wymiary","Jednostka","","Szerokość","mm","600"]
["","","","Głębokość","mm","728"]
["","","","Wysokość","mm","1,730"]
["Obudowa","Materiał","","","","Arkusz metalowy z powłoką wstępną"]
["","Kolor","","","","Biały"]
["Zbiornik","Objętość wody","","","l","180"]
["","Zabezpieczenie przed korozją","","","","Anoda"]
["","Izolacja","","Straty ciepła","kWh/24h","1.36 (4)"]
["Ciężar","Jednostka","","","kg","210"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","ηs (sprawność sezonowa ogrzewania pomieszczeń)","%","194"]
["","","","Klasa efektywności sezon. ogrzewania pomieszczeń","","A+++"]
["","","","SCOP","","5.06"]
["","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Seasonal space heating eff. class","","A++"]
["","","","ηs (sprawność sezonowa ogrzewania pomieszczeń)","%","139"]
["","","","SCOP","","3.68"]
["Wydajność grzewcza","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Maks.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","liczba faz","","","","3~"]
["","Nazwa","","","","9W"]
["","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","400"]
["Prąd","zalecane bezpieczniki","","","A","25"]
["Uwagi","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(3) - z glikolem propylenowym 40%"]
["","","","","","(4) - Straty ciepła według EN12897"]
["","","","","","(5) - Łącznie z instalacją + PHE + dodatkową grzałką; bez przeponowego naczynia wzbiorczego"]
["","","","","","(6) - Poziom ciśnienia akustycznego jest mierzony za pomocą mikrofonu z odległości 1 m od jednostki. Jest to wartość względna, zależy od odległości i warunków akustycznych."]
["","","","","","(7) - Przez pompę ciepła"]
["","","","","","(8) - Przez pompę ciepła + dodatkowy element grzewczy"]
["","","","","","(9) - Przez dodatkowy element grzewczy"]