{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Obudowa","Kolor","","","","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)","Biały (RAL9016) / Ciemno-szary (RAL7011)"]
["","Materiał","","","","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia"]
["Wymiary","Jednostka","","Wysokość","mm","1891","1896","1891","1896"]
["","","","Szerokość","mm","595","790","595","790"]
["","","","Głębokość","mm","615","790","615","790"]
["Ciężar","Jednostka","","","kg__","73.0","93.0","73.0","93.0"]
["PED","Kategoria","","","","art. 3.3","art. 3.3","art. 3.3","art. 3.3"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0"]
["","Ilość","","","kg__","1.50","1.50","1.50","1.50"]
["Poziom mocy akustycznej","Nom.","","","dBA","39","39","39","39"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65"]
["","Chłodzenie","Temp. otoczenia","Min.","°CDB","10","10","10","10"]
["","","Strona wodna","Min.","°C","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","230","230","230","230"]
["Grzałka elektryczna","Zasilanie","","Nazwa","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Faza","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Częstotliwość","Hz","50","50","50","50"]
["Uwagi","","","","","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","","(5) - Podgrzewanie zbiornika tylko przy pomocy pompy ciepła, nie podgrzewacza elektrycznego","","(5) - Podgrzewanie zbiornika tylko przy pomocy pompy ciepła, nie podgrzewacza elektrycznego"]