{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E"]
[]
[]
[]
[]
["","","","","","EHSX04P30EF","EHSX04P50EF","EHSX04P50EG","EHSX04P30EG","EHSX08P30EF","EHSX08P50EF","EHSX08P50EG","EHSX08P30EG"]
["Obudowa","Kolor","","","","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)","Biały (RAL9016) / Czarny (RAL9017)"]
["","Materiał","","","","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia","Polipropylen odporny na uderzenia"]
["Wymiary","Jednostka","","Wysokość","mm","1,892","1,905","1,910","1,891","1,892","1,905","1,910","1,891"]
["","","","Szerokość","mm","594","792","792","594","594","792","792","594"]
["","","","Głębokość","mm","644","812","817","644","644","812","817","644"]
["Ciężar","Jednostka","","","kg","77","107","97.0","77.0","77","107","97.0","77.0"]
["PED","Kategoria","","","","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3","Art. 4.3"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675","675.0","675.0","675","675","675.0","675.0"]
["","Ilość","","","kg","1.5","1.5","1.50","1.50","1.5","1.5","1.50","1.50"]
["Poziom mocy akustycznej","Nom.","","","dBA","39","39","39","39","39","39","39","39"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65","65","65","65","65"]
["","Chłodzenie","Temp. otoczenia","Min.","°CDB","10","10","10","10","10","10","10","10"]
["","","Strona wodna","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22","22","22","22","22"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50","50","50","50"]
["","Napięcie","","","V","230","230","230","230","230","230","230","230"]
["Uwagi","","","","","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897","(1) - Straty ciepła według EN12897"]