{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6VG / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVX04S23EA6VG / ERGA04EAV37","EHVX04S18EA6VG / ERGA04EAV37"]
["Wydajność grzewcza","Nom.","","","kW","4.36, 4.60","4.36, 4.60"]
["Wydajność chłodnicza","Nom.","","","kW","4.86, 4.52","4.86, 4.52"]
["Pobór mocy","Grzanie","","Nom.","kW","0.830, 1.26","0.830, 1.26"]
["","Chłodzenie","","Nom.","kW","0.810, 1.36","0.810, 1.36"]
["","Ciepła woda o temperaturze od 10°C do 50°C","","Nom.","kWh","3.01","2.48"]
["Czas nagrzewania od 10°C do 50°C","hr","","","","1h 40min","1h 28min"]
["COP","","","","","5.23, 3.65","5.23, 3.65"]
["EER","","","","","5.98, 3.32","5.98, 3.32"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","XL","L"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","A","A"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","3.29","3.29"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A++","A++"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 35°C","Informacje ogólne","SCOP","","4.96","4.96"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","A+++","A+++"]
["Uwagi","","","","","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]