{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","EHYHBH05AFV32","EHYHBH05AAV32","EHYHBH08AFV32","EHYHBH08AAV32"]
["Obudowa","Kolor","","","","Biały","Biały","Biały","Biały"]
["","Materiał","","","","Arkusz metalowy z powłoką wstępną","Arkusz metalowy z powłoką wstępną","Arkusz metalowy z powłoką wstępną","Arkusz metalowy z powłoką wstępną"]
["Wymiary","Jednostka","","Wysokość","mm","902","902","902","902"]
["","","","Szerokość","mm","450","450","450","450"]
["","","","Głębokość","mm","164","164","164","164"]
["Ciężar","Jednostka","","","kg","30.0","30.0","31.2","31.2"]
["PED","Kategoria","","","","Art 3 §3:, Określenie wartości granicznych dla prądów harm. wytwarzanych przez sprzęt podłączony do publ. sieci niskiego napięcia","Art 3 §3:, Określenie wartości granicznych dla prądów harm. wytwarzanych przez sprzęt podłączony do publ. sieci niskiego napięcia","Kategoria I","Kategoria I"]
["Strona wodna wymiennika ciepła","Natężenie przepływu wody","Ogrzewanie","Maks.","l/min","23.0 (7)","23.0","23.5 (7)","23.5"]
["Poziom mocy akustycznej","Nom.","","","dBA","42.0","42.0","42.0","42.0"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","25 (8)","25","25 (8)","25"]
["","","","Maks.","°C","55 (8)","55","55 (8)","55"]
["Zasilanie energią elektryczną","Nazwa","","","","V3","V3","V3","V3"]
["","liczba faz","","","","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","230","230","230","230"]
["Złącza przewodów","Do połączenia z interfejsem użytkownika","","ilość","","2","2","2","2"]
["","","","Uwaga","","0,75 mm² do 1,25 mm² (maks. długość 500 m)","0,75 mm² do 1,25 mm² (maks. długość 500 m)","0,75 mm² do 1,25 mm² (maks. długość 500 m)","0,75 mm² do 1,25 mm² (maks. długość 500 m)"]
["Uwagi","","","","","(1) - Tylko dla jednostki wewnętrznej","","(1) - Tylko dla jednostki wewnętrznej"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), z obejściem kotła","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), z obejściem kotła"]
["","","","","","(4) - Min. required","","(4) - Min. required"]
["","","","","","(5) - Z obejściem kotła","","(5) - Z obejściem kotła"]
["","","","","","(6) - Zakres pracy *HYHB* i *HYKOMB33AA, zob. rysunek zakresu pracy","","(6) - Zakres pracy *HYHB* i *HYKOMB33AA, zob. rysunek zakresu pracy"]