{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AAV3 / EVLQ08CAV3","EHYHBX08AFV3 / EVLQ08CAV3"]
["Podgrzewanie ciepłej wody użytkowej","Ogólny","","Zadeklarowany profil obciążenia","","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","A"]
["COP","","","","","4.45 (3), 3.42 (4)","4.45, 3.42"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Seasonal space heating eff. class","","A++"]
["","","","ηs (sprawność sezonowa ogrzewania pomieszczeń)","%","129"]
["","","","SCOP","","3.29"]
["Wydajność chłodnicza","Nom.","","","kW","6.86 (4), 5.36 (4)"]
["","Min.","","","kW","2.50 (3), 2.50 (4)"]
["EER","","","","","3.42 (3), 2.29 (4)","3.42, 2.29"]
["Wydajność grzewcza","Nom.","","","kW","7.40 (3), 6.89 (4)"]
["","Min.","","","kW","1.80 (3), 1.80 (4)"]
["","Maks.","","","kW","10.0 (3), 9.53 (4)"]
["Power input","Chłodzenie","","Nom.","kW","2.01 (3), 2.34 (4)"]
["","Grzanie","","Nom.","kW","1.66 (3), 2.01 (4)"]
["Uwagi","","","","","(1) - Warunek: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Warunek: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - Warunek 1: chłodzenie Ta 35°C - LWE 18°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Temp. otocz. 35°C - LWE 7℃ (DT=5°C), kocioł zbocznikowany"]
["","","","","","(4) - Warunek 2: chłodzenie Ta 35°C - LWE 7°C (DT = 5°C); ogrzewanie Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(4) - Temp. otocz. 35°C - LWE 18℃ (DT=5°C), kocioł zbocznikowany"]
["","","","","","(5) - Temp. otocz. 35°C - LWE 7℃ (DT=5°C), kocioł zbocznikowany","(5) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła"]
["","","","","","(6) - Temp. otocz. 35°C - LWE 18℃ (DT=5°C), kocioł zbocznikowany","(6) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), z obejściem kotła"]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła"]
["","","","","","(8) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), z obejściem kotła"]
["Wydajność grzewcza","Min.","","","kW","","1.80, 1.80"]
["","Nom.","","","kW","","7.40, 6.89"]
["","Maks.","","","kW","","10.0, 9.53"]
["Wydajność chłodnicza","Min.","","","kW","","2.50, 2.50"]
["","Nom.","","","kW","","6.86, 5.36"]
["Pobór mocy","Grzanie","","Nom.","kW","","1.66, 2.01"]
["","Chłodzenie","","Nom.","kW","","2.01, 2.34"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","","XL"]
["","Klimat umiarkowany","","Grzanie wody, klasa efektywności energetycznej","","","A"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 55°C","Informacje ogólne","SCOP","","","3.29"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 55°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","A++"]
["Ogrzewanie pomieszczeń","Temp. wylot. wody dla przeciętnych warunków klimatycznych 35°C","Informacje ogólne","SCOP","","","4.28"]
["Ogrz. pom.","Temp. wy. wody dla przec. war. klim. 35°C","Informacje ogólne","Klasa efektywności sezon. ogrzewania pomieszczeń","","","A++"]
["Zakres efektywności energetycznej","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]