{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Obudowa","Kolor","","","","Biały"]
["","Materiał","","","","Arkusz metalowy z powłoką wstępną"]
["Wymiary","Jednostka","","Wysokość","mm","902"]
["","","","Szerokość","mm","450"]
["","","","Głębokość","mm","164"]
["Ciężar","Jednostka","","","kg","31.2"]
["PED","Kategoria","","","","Kategoria I"]
["Strona wodna wymiennika ciepła","Natężenie przepływu wody","Ogrzewanie","Maks.","l/min","23.5 (7)"]
["Poziom mocy akustycznej","Nom.","","","dBA","42.0"]
["Zakres pracy","Grzanie","Strona wodna","Min.","°C","25 (8)"]
["","","","Maks.","°C","55 (8)"]
["","Chłodzenie","Temp. otoczenia","Min.","°CDB","10 (8)"]
["","","Strona wodna","Min.","°C","5 (8)"]
["","","","Maks.","°C","22 (8)"]
["Zasilanie energią elektryczną","Nazwa","","","","V3"]
["","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","230"]
["Złącza przewodów","Do połączenia z interfejsem użytkownika","","ilość","","2"]
["","","","Uwaga","","0,75 mm² do 1,25 mm² (maks. długość 500 m)"]
["Uwagi","","","","","(1) - Tylko dla jednostki wewnętrznej"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), z obejściem kotła"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), z obejściem kotła"]
["","","","","","(4) - Temp. otocz. 35°C - LWE 7℃ (DT=5°C), kocioł zbocznikowany"]
["","","","","","(5) - Temp. otocz. 35°C - LWE 18℃ (DT=5°C), kocioł zbocznikowany"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Z obejściem kotła"]
["","","","","","(8) - Zakres pracy *HYHB* i *HYKOMB33AA, zob. rysunek zakresu pracy"]