{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA3"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA3"]
["Gaz","Złącze","","Średnica","mm","15"]
["","Zużycie (G20)","","Min.","m³/h","0.79"]
["","","","Maks.","m³/h","3.39"]
["","Zużycie (G25)","","Min.","m³/h","0.89"]
["","","","Maks.","m³/h","3.92"]
["","Zużycie (G31)","","Min.","m³/h","0.30"]
["","","","Maks.","m³/h","1.29"]
["","Klasa NOx","","","","6"]
["","Poziom NOx (G20)","","","mg/kWh","36"]
["Centralne ogrzewanie","Doprowadzone ciepło Qn (wartość opałowa dolna)","Nom.","Min.","kW","7.6"]
["","","","Maks.","kW","27.0"]
["","","","Min.","kW","8.4"]
["","","","Maks.","kW","30.0"]
["","Moc wyjściowa Pn w temp. 80/60°C","","Min.","kW","7.5"]
["","","","Nom.","kW","26.6"]
["","Moc wyjściowa Pn w temp. 37/30°C","","Nom.","kW","8.2"]
["","Temperatura wody","","Maks.","°C","90"]
["Ciepła woda użytkowa","Doprowadzone ciepło (wartość opałowa dolna) Qnw","Nom.","Min.","kW","7.6"]
["","","","Maks.","kW","32.7"]
["","","","Min.","kW","8.4"]
["","","","Maks.","kW","36.3"]
["","Klasa komfortu (EN13203)","","","","XL"]
["","Temperatura","","Maks.","°C","65"]
["Powietrze zasilające","Współśrodkowe","","","","Nie"]
["Gazy spalinowe","Temperatura","","Maks.","°C","70"]
["","Przyłącze","","","mm","60"]
["","Przepływ masowy (G20)","","Maks.","kg/h","54.4"]
["","Przepływ masowy (G25)","","Maks.","kg/h","54.4"]
["","Przepływ masowy (G31)","","Maks.","kg/h","53.6"]
["Obudowa","Kolor","","","","BIAŁY (RAL 9010)"]
["","Materiał","","","","Arkusz metalowy z powłoką wstępną"]
["Wymiary","Jednostka","Wysokość","Obudowa","mm","710"]
["","","","Szerokość","mm","450"]
["","","","Głębokość","mm","240"]
["Ciężar","Jednostka","","Pusty","kg","36"]
["Ciepła woda użytkowa i grzanie","Informacje ogólne","","Zadeklarowany profil obciążenia","","XL"]
["Podgrzew ciepłej wody użytkowej","Informacje ogólne","","Klasa efektywności energetycznej podgrzewu wody","","A"]
["Ogrzewanie pomieszczeń","Informacje ogólne","","Klasa sezonowej efek. ogrzewania pomieszczeń","","A"]